{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","47"]
["","Rafraîchissement","","Nom.","dBA","46"]
["Accessoires standard","Manuel d'installation","","","","1"]
["","Sachet de vis","","","","1"]
["","Bouchon d'évacuation","","","","1"]
["","Bouchon d'évacuation (1)","","","","6"]
["","Bouchon d'évacuation (2)","","","","3"]
["","Étiquette F-Gas détachable","","","","1"]
["","Étiquette supplémentaire de réfrigérant","","","","1"]
["Réfrigérant","Charge","","","TCO2Eq","1.2"]
["","PRP","","","","675"]
["","Charge","","","kg","1.8"]
["","Type","","","","R-32"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","420"]
["","","Chauffage","Très lent","tr/min","420"]
["Raccords de tuyauterie","Dénivelé","UI - UI","Max.","m","7.5"]
["","","UI - UE","Max.","m","15"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 30 m)"]
["","Longueur totale de tuyauterie","Système","Réel","m","50"]
["Compresseur","Type","","","","Compresseur swing hermétique"]
["Dimensions","Unité","","Largeur","mm","868"]
["","","","Profondeur","mm","320"]
["","","","Hauteur","mm","734"]
["Poids","Unité","","","kg","57"]
["Power supply","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","220-240"]
["Remarques","","","","","(1) - Contient des gaz à effet de serre fluorés."]
["","","","","","(2) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(3) - Pour les données électriques, se reporter au schéma séparé."]
["Ventilateur","Débit d’air","Rafraîchissement","Extra lent","m³/min","","24"]
["","","Chauffage","Très lent","m³/min","","24"]
["","","","Extra lent","cfm","","847"]
["","","Chauffage","Très lent","cfm","","847"]
["Dimensions","Unité","","Hauteur","mm","","734"]
["","","","Largeur","mm","","868"]
["","","","Profondeur","mm","","320"]
["Poids","Unité","","","kg","","57"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","","420"]
["","","Chauffage","Très lent","tr/min","","420"]
["Compresseur","Type","","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","","-10"]
["","","","Max.","°CBS","","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","","-15"]
["","","","Max.","°CBH","","18"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","","46"]
["","Chauffage","","Nom.","dBA","","47"]
["Réfrigérant","","","","","","R-32"]
["","Charge","","","kg","","1.80"]
["","Charge","","","tCO2Eq","","1.2"]
["","Réfrigérant-=-PRP","","","","","675"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","","25"]
["","Charge de réfrigérant supplémentaire","","","kg/m","","0,02 (pour longueur de tuyauterie supérieure à 30 m)"]
["","Dénivelé","UI - UE","Max.","m","","15"]
["","","UI - UI","Max.","m","","7.5"]
["","Longueur totale de tuyauterie","Système","Réel","m","","50"]
["Accessoires standard","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Alimentation électrique","Phase","","","","","1~"]
["","Fréquence","","","Hz","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","220-240"]