{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N8"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B8","3MXM52N2V1B8"]
["Dimensions","Unité","","Hauteur","mm","734","734"]
["","","","Largeur","mm","974","974"]
["","","","Profondeur","mm","401","401"]
["Poids","Unité","","","kg","57","57"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","420","420"]
["","","Chauffage","Très lent","tr/min","420","420"]
["Compressor","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10","-10"]
["","","","Max.","°CBS","46","46"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","46","46"]
["","Chauffage","","Nom.","dBA","47.0","47.0"]
["Réfrigérant","","","","","R-32","R-32"]
["","Charge","","","kg","1.8","1.8"]
["","Charge","","","tCO2Eq","1.22","1.22"]
["","Réfrigérant-=-PRP","","","","675.0","675.0"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","25","25"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 30 m)","0,02 (pour longueur de tuyauterie supérieure à 30 m)"]
["","Dénivelé","UI - UE","Max.","m","15.0","15.0"]
["","","UI - UI","Max.","m","7.5","7.5"]
["","Longueur totale de tuyauterie","Système","Réel","m","50","50"]
["Accessoires standard","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240"]
["Remarques","","","","","(1) - Par pièce","(1) - Par pièce"]
["","","","","","(2) - Pour combinaison avec CVXM-A, FVXM-A - la longueur maximale de tuyauterie est 30 m.","(2) - Pour combinaison avec CVXM-A, FVXM-A - la longueur maximale de tuyauterie est 30 m."]