{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":8,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-E"]
[]
[]
[]
[]
["","","","","","3MXS52E4V1B2","3MXS52E4V1B","3MXS52E3V1B"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","47","47"]
["","Rafraîchissement","","Nom.","dBA","46","46"]
["Accessoires standard","Manuel d'installation","","","","1","1"]
["","Bouchon d'évacuation","","","","1","1"]
["","Réducteur","","","","1","1"]
["","Plaque de réglage de direction d'air","","","","1","1"]
["Réfrigérant","Charge","","","TCO2Eq","4.2","4.2"]
["","PRP","","","","2,087.5","2,087.5"]
["","Charge","","","kg","2.0","2.0"]
["","Type","","","","R-410A","R-410A"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Max.","°CBS","46","46"]
["","","","Min.","°CBS","-10","-10"]
["","Chauffage","Extérieure","Max.","°CBH","18","18"]
["","","","Min.","°CBH","-15","-15"]
["Raccords de tuyauterie","Dénivelé","UI - UI","Max.","m","7.5","7.5"]
["","","UI - UE","Max.","m","15","15"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 30 m)","0,02 (pour longueur de tuyauterie supérieure à 30 m)"]
["","Longueur totale de tuyauterie","Système","Réel","m","50","50"]
["Compressor","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Dimensions","Unité","","Largeur","mm","936","936"]
["","","","Profondeur","mm","300","300"]
["","","","Hauteur","mm","735","735"]
["Poids","Unité","","","kg","49","49"]
["Power supply","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Tension","","","V","230","230"]
["Remarques","","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35°CBS; longueur de tuyauterie équivalente : 7,5m","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35°CBS; longueur de tuyauterie équivalente : 7,5m"]
["","","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m"]
["","","","","","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés."]
["Dimensions","Unité","","Hauteur","mm","","","735"]
["","","","Largeur","mm","","","936"]
["","","","Profondeur","mm","","","300"]
["Poids","Unité","","","kg","","","49"]
["Compressor","Type","","","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","","","-10"]
["","","","Max.","°CBS","","","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","","","-15"]
["","","","Max.","°CBH","","","15.5"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","","","46"]
["","Chauffage","","Nom.","dBA","","","47"]
["Réfrigérant","","","","","","","R-410A"]
["","Charge","","","kg","","","2.0"]
["","Charge","","","tCO2Eq","","","4.2"]
["","Réfrigérant-=-PRP","","","","","","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","","","25"]
["","Charge de réfrigérant supplémentaire","","","kg/m","","","0,02 (pour longueur de tuyauterie supérieure à 30 m)"]
["","Dénivelé","UI - UE","Max.","m","","","15"]
["","","UI - UI","Max.","m","","","7.5"]
["","Longueur totale de tuyauterie","Système","Réel","m","","","50"]
["Accessoires standard","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["","Air direction adjustment plate","","","","","","1"]
["Alimentation électrique","Phase","","","","","","1~"]
["","Fréquence","","","Hz","","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","","230"]