{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":7,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXD-A"]
[]
[]
[]
[]
["","","","","","ATXD25A5V1B","ATXD35A5V1B"]
["Power input","Rafraîchissement","","Nom.","kW","","0.032"]
["","Chauffage","","Nom.","kW","","0.032"]
["Caisson","Couleur","","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","","286"]
["","","","Largeur","mm","","770"]
["","","","Profondeur","mm","","225"]
["Poids","Unité","","","kg","","9.00"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","11.0"]
["","","","Moyen","m³/min","","8.5"]
["","","","Bas","m³/min","","6.8"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","5.4"]
["","","Chauffage","Haut","m³/min","","11.5"]
["","","","Moyen","m³/min","","9.4"]
["","","","Bas","m³/min","","7.7"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","6.3"]
["Sound power level","Rafraîchissement","","","dBA","","58"]
["","Chauffage","","","dBA","","58"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","43"]
["","","","Moyen","dBA","","34"]
["","","","Bas","dBA","","27"]
["","","","Faible niveau sonore de fonctionnement","dBA","","20"]
["","Chauffage","","Haut","dBA","","40"]
["","","","Moyen","dBA","","35"]
["","","","Bas","dBA","","29"]
["","","","Faible niveau sonore de fonctionnement","dBA","","21"]
["Raccordements de tuyauterie","Liquide","","DE","mm","","6"]
["","Gaz","","DE","mm","","9.50"]
["","Évacuation","","","","","18"]
["Systèmes de commande","Infrared remote control","","","","","ARC480A78"]
["","Télécommande câblée","","","","","BRC944B2, BRC073A1"]
["Accessoires standard","Manuel d'installation","","","","","1"]
["","Manuel d’utilisation","","","","","1"]
["","Télécommande infrarouge","","","","","1"]
["","Piles sèches AAA","","","","","2"]
["","Support de télécommande","","","","","1"]
["","Plaque de montage","","","","","1"]
["","Filtre désodorisant à apatite de titane","","","","","1"]
["","Filtre à particules argent","","","","","1"]
["","Vis de fixation d'unité intérieure","","","","","2"]
["","Précautions générales de sécurité","","","","","1"]
["Power supply","Phase","","","","","1~"]
["","Fréquence","","","Hz","","50"]
["","Tension","","","V","","220-240"]
["Remarques","","","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 5m ; dénivelé : 0m"]
["","","","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m (horizontale)"]
["","","","","","","(3) - Pour les données électriques, se reporter au schéma séparé."]
["Niveau de puissance sonore","Chauffage","","","dBA","55"]
["","Rafraîchissement","","","dBA","55"]
["Dimensions","Unité","","Hauteur","mm","286"]
["","","","Largeur","mm","770"]
["","","","Profondeur","mm","225"]
["Poids","Unité","","","kg","8.5"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","40"]
["","","","Bas","dBA","26"]
["","Chauffage","","Haut","dBA","40"]
["","","","Bas","dBA","28"]
["Accessoires standard","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Alimentation électrique","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240"]