{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-A9"]
[]
[]
[]
[]
["","","","","ATXM35R2V1B / ARXM35A5V1B9","ATXM35R5V1B / ARXM35A5V1B9"]
["Puissance frigorifique","Min.","","kW","1.4","1.4"]
["","Nom.","","kW","3.4","3.4"]
["","Max.","","kW","4","4"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","1.4","1.4"]
["","Nom.","","kW","4","4"]
["","Max.","","kW","5.2","5.2"]
["Efficacité nominale","EER","","","4.23","4.23"]
["","COP","","","4.04","4.04"]
["","Consommation énergétique annuelle","","kWh","402","402"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A+++","A+++"]
["","Puissance","Pdesign","kW","3.4","3.4"]
["","SEER","","","8.55","8.55"]
["","Consommation d’énergie annuelle","","kWh/a","139","139"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A+++","A+++"]
["","Puissance","Pdesign","kW","2.5","2.5"]
["","SCOP/A","","","5.1","5.1"]
["","Pdh Puissance calorifique à -10°","","kW","2.35","2.35"]
["","Consommation d’énergie annuelle","","kWh/a","686","686"]
["Classe d'efficacité énergétique","","","","A+++ ~ D","A+++ ~ D"]
["Remarques","","","","(1) - Voir le schéma séparé pour la plage de fonctionnement","(1) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","(2) - Pour les données électriques, se reporter au schéma séparé.","(2) - Pour les données électriques, se reporter au schéma séparé."]
["","","","","(3) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes: température intérieure: 27°CBS, 19°CBH; température extérieure: 35°CBS ; longueur équivalente de tuyauterie de réfrigérant: 5m, dénivellation: 0m.","(3) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes: température intérieure: 27°CBS, 19°CBH; température extérieure: 35°CBS ; longueur équivalente de tuyauterie de réfrigérant: 5m, dénivellation: 0m."]
["","","","","(4) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes: température intérieure: 20°CBS; température extérieure: 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente: 5m, dénivelé: 0m.","(4) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes: température intérieure: 20°CBS; température extérieure: 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente: 5m, dénivelé: 0m."]