{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":95,"n_cols":13,"rows_kept":95,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B","ATXM20R5V1B","ATXM25R2V1B","ATXM25R5V1B","ATXM35R2V1B","ATXM35R5V1B","ATXM50R2V1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","39"]
["","","","Moyen","dBA","34"]
["","","","Faible niveau sonore de fonctionnement","dBA","20"]
["","","","Bas","dBA","26"]
["","Rafraîchissement","","Moyen","dBA","33"]
["","","","Faible niveau sonore de fonctionnement","dBA","19"]
["","","","Bas","dBA","25"]
["","","","Haut","dBA","41"]
["Accessoires standard","Manuel d'installation","","","","1"]
["","Manuel d’utilisation","","","","1"]
["","Télécommande infrarouge","","","","1"]
["","Piles sèches AAA","","","","2"]
["","Support de télécommande","","","","1"]
["","Plaque de montage","","","","1"]
["","Filtre désodorisant à apatite de titane","","","","1"]
["","Vis de fixation d'unité intérieure","","","","2"]
["","Kit d'adaptateur WLAN","","","","1"]
["Systèmes de commande","Télécommande câblée","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Raccordements de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","9.50"]
["","Évacuation","","","","18"]
["Power input","Rafraîchissement","","Nom.","kW","0.029"]
["","Chauffage","","Nom.","kW","0.023"]
["Sound power level","Rafraîchissement","","","dBA","58"]
["","Chauffage","","","dBA","55"]
["Dimensions","Unité","","Largeur","mm","778"]
["","","","Profondeur","mm","272"]
["","","","Hauteur","mm","295"]
["Caisson","Couleur","","","","Blanc"]
["Poids","Unité","","","kg","10.0"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","9.3"]
["","","","Moyen","m³/min","8.2"]
["","","","Bas","m³/min","6.2"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.1"]
["","","Rafraîchissement","Bas","m³/min","5.7"]
["","","","Moyen","m³/min","7.5"]
["","","","Haut","m³/min","10.5"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.3"]
["Power supply","Phase","","","","1~"]
["","Nom","","","","V1"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","220-240"]
["Remarques","","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m"]
["","","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Chauffage","","Nom.","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Caisson","Couleur","","","","","Blanc","Blanc","Blanc","Blanc","Blanc","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","","295","295","295","295","295","295","299"]
["","","","Largeur","mm","","778","778","778","778","778","778","998"]
["","","","Profondeur","mm","","272","272","272","272","272","272","292"]
["Poids","Unité","","","kg","","10","10","10","10","10","10","14.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Chauffage","Haut","m³/min","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","8.2","8.2","8","8","8.5","8.5","14.2"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","58","58","58","58","58","58","58"]
["","Chauffage","","","dBA","","55","55","55","55","55","55","58"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","41","41","41","41","45","45","44"]
["","Refroidissement","","Moyen","dBA","","33","33","33","33","33","33","40"]
["","","","Bas","dBA","","25","25","25","25","25","25","36"]
["","","","Faible niveau sonore de fonctionnement","dBA","","19","19","19","19","19","19","27"]
["","Chauffage","","Haut","dBA","","39","39","39","39","39","39","43"]
["","","","Moyen","dBA","","34","34","34","34","35","35","39"]
["","","","Bas","dBA","","26","26","27","27","28","28","34"]
["","","","Faible niveau sonore de fonctionnement","dBA","","20","20","20","20","20","20","31"]
["Raccords de tuyauterie","Liquide","","DE","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gaz","","DE","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Évacuation","","","","","18","18","18","18","18","18","18"]
["Systèmes de commande","Infrared remote control","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["Systèmes de commande","Télécommande câblée","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Accessoires standard","Installation manual","","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","1","1"]
["Alimentation électrique","Nom","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Phase","","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","","50","50","50","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Accessoires standard","Silver particle filter","","","","","","","","","","","1"]