{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MY1"]
[]
[]
[]
[]
["","","","","","AZAS125M7Y1B","AZAS100M7Y1B (Archived)","AZAS140M7Y1B (Archived)"]
["Dimensions","Unité","","Hauteur","mm","990","990","990"]
["","","","Largeur","mm","940","940","940"]
["","","","Profondeur","mm","320","320","320"]
["Poids","Unité","","","kg","70"]
["Compresseur","Type","","","","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-5","-5","-5"]
["","","","Max.","°CBS","46","46","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","-15","-15","-15"]
["","","","Max.","°CBH","15.5","15.5","15.5"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","71","70","73"]
["","Chauffage","","","dBA","71","","73 (1)"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","53","53","54"]
["","Chauffage","","Nom.","dBA","57","57","57"]
["Réfrigérant","Type","","","","R-32"]
["","Charge","","","kg","2.60","2.60","2.90"]
["Réfrigérant","PRP","","","","675"]
["Réfrigérant","Charge","","","tCO2Eq","1.76","1.76","1.96"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52","9.52","9.52"]
["Raccordements de tuyauterie","Gaz","","DE","mm","15.9"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","30","30","30"]
["","","Système","Équivalente","m","50","50","50"]
["","","","Préchargé d'usine jusqu'à","m","30","30","30"]
["","Charge de réfrigérant supplémentaire","","","kg/m","Voir le manuel d'installation","Voir le manuel d'installation","Voir le manuel d'installation"]
["","Dénivelé","UI - UE","Max.","m","30.0","30.0","30.0"]
["","","UI - UI","Max.","m","0.5","0.5","0.5"]
["Accessoires standard","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Alimentation électrique","Phase","","","","3~","3~","3~"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","50","50","50"]
["","Alimentation électrique-=-Tension","","Alimentation électrique-=-Tension-=-V","","380-415","380-415","380-415"]
["Courant - 50&nbsp;Hz","Courant - 50&nbsp;Hz-=-Intensité maximum de fusible (MFA)","","Courant - 50&nbsp;Hz-=-Intensité maximum de fusible (MFA)-=-A","","16"]
["Remarques","","","","","(1) - Conforme à la norme ENER Lot 21","","(1) - Conforme à la norme ENER Lot 21"]
["Poids","Unité","","","kg","","70","77"]
["Compresseur","Type","","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Réfrigérant","","","","","","R-32","R-32"]
["","Réfrigérant-=-PRP","","","","","675","675"]
["Raccords de tuyauterie","Gaz","","DE","mm","","15.9","15.9"]
["Courant&nbsp;- 50&nbsp;Hz","Courant&nbsp;- 50&nbsp;Hz-=-Intensité maximale de fusible (MFA)-=-A","","","A","","16","16"]