{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BAEF125AWB"]
[]
[]
[]
[]
["","","","","BAEF125AWB."]
["Puissance absorbée","kW","","","0.006"]
["Caisson","Couleur","","","Gray"]
["","DEL de fonctionnement","Couleur","","Blue/red"]
["Dimensions","Unité","Hauteur","mm","100"]
["","","Largeur","mm","840"]
["","","Profondeur","mm","840"]
["","Unité emballée","Hauteur","mm","168"]
["","","Largeur","mm","910"]
["","","Profondeur","mm","910"]
["Poids","Unité","","kg","12.0"]
["","Unité emballée","","kg","15.5"]
["Emballage","Matériau","","","Carton"]
["","Poids","","kg","4"]
["Power supply","Phase","","","1~"]
["","Fréquence","","Hz","50/60"]
["","Tension","","V","220-240/220"]
["Remarques","","","","(1) - Avec 2 capteurs (facteur de contrôle 0,65) : A+ ; Autres : A"]