{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AW"]
[]
[]
[]
[]
["","","","","","CTXA15A2V1BW"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","39"]
["","","","Moyen","dBA","32"]
["","","","Faible niveau sonore de fonctionnement","dBA","21"]
["","","","Bas","dBA","25"]
["","Rafraîchissement","","Moyen","dBA","32"]
["","","","Faible niveau sonore de fonctionnement","dBA","21"]
["","","","Bas","dBA","25"]
["","","","Haut","dBA","39"]
["Accessoires standard","Manuel d'installation","","","","1"]
["","Manuel d’utilisation","","","","1"]
["","Filtre à air","","","","2"]
["","Télécommande infrarouge","","","","1"]
["","Plaque de montage de télécommande","","","","1"]
["","Sachet de vis","","","","1"]
["","Cache de vis","","","","1"]
["","Piles sèches AAA","","","","2"]
["","Précautions générales de sécurité","","","","1"]
["Réfrigérant","PRP","","","","675.0"]
["Systèmes de contrôle","Télécommande câblée","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","9.50"]
["","Évacuation","","","","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.020"]
["","Chauffage","","Nom.","kW","0.020"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","57"]
["Dimensions","Unité","","Largeur","mm","798"]
["","","","Profondeur","mm","189"]
["","","","Hauteur","mm","295"]
["Caisson","Couleur","","","","Blanc"]
["Poids","Unité","","","kg","12"]
["Ventilateur","Débit d’air","Chauffage","Haut","m³/min","10.9"]
["","","","Moyen","m³/min","8.7"]
["","","","Bas","m³/min","6.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.5"]
["","","Rafraîchissement","Bas","m³/min","6.1"]
["","","","Moyen","m³/min","8"]
["","","","Haut","m³/min","11.0"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.6"]
["Power supply","Phase","","","","1~"]
["","Nom","","","","V1"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","220-240"]