{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":7,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-A"]
[]
[]
[]
[]
["","","","","","CTXM15A5V1B (Archived)","CTXM15A2V1B (Archived)"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.019","0.019"]
["","Chauffage","","Nom.","kW","0.018","0.018"]
["Caisson","Couleur","","","","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","298","298"]
["","","","Largeur","mm","804","804"]
["","","","Profondeur","mm","252","252"]
["Poids","Unité","","","kg","11.5","11.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","11.9","11.9"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","8.9","8.9"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","6.3","6.3"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.9","4.9"]
["","","Chauffage","Haut","m³/min","11.4","11.4"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","9.2","9.2"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","6.9","6.9"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.9","4.9"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","54","54"]
["","Chauffage","","","dBA","53","53"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","41","41"]
["","Refroidissement","","Moyen","dBA","33","33"]
["","","","Bas","dBA","25","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19"]
["","Chauffage","","Haut","dBA","39","39"]
["","","","Moyen","dBA","34","34"]
["","","","Bas","dBA","26","26"]
["","","","Faible niveau sonore de fonctionnement","dBA","20","20"]
["Réfrigérant","Réfrigérant-=-PRP","","","","675","675"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.4","6.4"]
["","Gaz","","DE","mm","9.5","9.5"]
["","Évacuation","","","","16","16"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC466A86","ARC466A86"]
["","Télécommande câblée","","","","BRC073A1","BRC073A1"]
["Accessoires standard","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Installation plate","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentation électrique","Nom","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240"]