{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.029","0.029"]
["","Chauffage","","Nom.","kW","0.023","0.023"]
["Caisson","Couleur","","","","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","295","295"]
["","","","Largeur","mm","778","778"]
["","","","Profondeur","mm","272","272"]
["Poids","Unité","","","kg","10","10"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","10.5","10.5"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","7.5","7.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","5.7","5.7"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.3","4.3"]
["","","Chauffage","Haut","m³/min","9.3","9.3"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","8.2","8.2"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","6.2","6.2"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.1","5.1"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","57","57"]
["","Chauffage","","","dBA","54","54"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","41","41"]
["","Refroidissement","","Moyen","dBA","33","33"]
["","","","Bas","dBA","25","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19"]
["","Chauffage","","Haut","dBA","39","39"]
["","","","Moyen","dBA","34","34"]
["","","","Bas","dBA","26","26"]
["","","","Faible niveau sonore de fonctionnement","dBA","20","20"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35"]
["","Gaz","","DE","mm","9.5","9.5"]
["","Évacuation","","","","18","18"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC466A67","ARC466A67"]
["Systèmes de commande","Télécommande câblée","","","","BRC073A1","BRC073A1"]
["Accessoires standard","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Alimentation électrique","Nom","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240"]