{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":8,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","38","","41"]
["","","","Faible niveau sonore de fonctionnement","dBA","21","","21"]
["","","","Bas","dBA","28","","30"]
["","Rafraîchissement","","Faible niveau sonore de fonctionnement","dBA","21","","21"]
["","","","Bas","dBA","25","","28"]
["","","","Haut","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Rafraîchissement","","Nom.","dBA","31","","35"]
["Accessoires standard","Manuel d'installation","","","","1","","1"]
["","Manuel d’utilisation","","","","1","","1"]
["","Télécommande infrarouge","","","","1","","1"]
["","Piles","","","","2","","2"]
["","Support de télécommande","","","","1","","1"]
["","Plaque de montage","","","","1","","1"]
["","Vis de fixation d'unité intérieure","","","","2","","2"]
["","Filtre purificateur d'air photocatalytique à apatite de titane","","","","2","","2"]
["Systèmes de commande","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","","6.35"]
["","Gaz","","DE","mm","9.5","","9.5"]
["","Évacuation","","","","18","","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.040","","0.040"]
["","Chauffage","","Nom.","kW","0.040","","0.040"]
["Sound power level","Rafraîchissement","","","dBA","55","","59"]
["","Chauffage","","","dBA","56","","58"]
["Dimensions","Unité","","Largeur","mm","780","","780"]
["","","","Profondeur","mm","215","","215"]
["","","","Hauteur","mm","289","","289"]
["Casing","Colour","","","","Blanc","","Blanc"]
["Poids","Unité","","","kg","8","","8"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","","","10.1"]
["","","","Bas","m³/min","","","6.3"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","","4.3"]
["","","Rafraîchissement","Bas","m³/min","","","5.2"]
["","","","Haut","m³/min","","","9.2"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Rafraîchissement","Nom.","m³/min","","","7.2"]
["Power supply","Phase","","","","1~","","1~"]
["","Fréquence","","","Hz","50","","50"]
["","Nom","","","","V1","","V1"]
["","Tension","","","V","220-240","","220-240"]
["Remarques","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","0.04"]
["","Chauffage","","Nom.","kW","","0.04"]
["Caisson","Couleur","","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","","289"]
["","","","Largeur","mm","","780"]
["","","","Profondeur","mm","","215"]
["Poids","Unité","","","kg","","8"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","7.9"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","6.3"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","4.7"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","3.9"]
["","","Chauffage","Haut","m³/min","","9"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","7.5"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","4.3"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","55"]
["","Chauffage","","","dBA","","56"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","37"]
["","Refroidissement","","Moyen","dBA","","31"]
["","","","Bas","dBA","","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","","21"]
["","Chauffage","","Haut","dBA","","38"]
["","","","Moyen","dBA","","33"]
["","","","Bas","dBA","","28"]
["","","","Faible niveau sonore de fonctionnement","dBA","","21"]
["Raccords de tuyauterie","Liquide","","DE","mm","","6.35"]
["","Gaz","","DE","mm","","9.5"]
["","Évacuation","","","","","18"]
["Systèmes de commande","Infrared remote control","","","","","ARC466A6"]
["Accessoires standard","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Alimentation électrique","Nom","","","","","V1"]
["","Phase","","","","","1~"]
["","Fréquence","","","Hz","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","220-240"]