{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":13,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2U50GC-A"]
[]
[]
[]
[]
["","","","","","D2U50GC015AB","D2U50GC020AB","D2U50GC024AB","D2U50GC028AB","D2U50GC015AA (Archived)","D2U50GC020AA (Archived)","D2U50GC024AA (Archived)","D2U50GC028AA (Archived)"]
["Pertes thermiques","Chaudière de réserve Ps","","","kW","0.0","0.0","0.0","0.0"]
["","Chaudière de réserve","","","kWh/24 h","","","","","1.7","1.7","1.7","1.7"]
["","Chaudière de réserve qS","","","kW","0.0","0.0","0.0","0.0"]
["Eau chaude sanitaire","Apport de chaleur (valeur calorifique brute) Qnw","Nom.","Max.","kW","16.7","22.2","26.6","31.1","16.7","22.2","26.6","31.1"]
["","","","Min.","kW","3.3","3.3","4.4","4.4","3.3","3.3","4.4","4.4"]
["","Sortie","","Min.","kW","3.0","3.0","4.0","4.0","3.0","3.0","4.0","4.0"]
["","Température","","Max.","°C","70","70","70","70","85","85","85","85"]
["","Apport de chaleur (valeur calorifique nette) Qnw","Nom.","Min.","kW","3.0","3.0","4.0","4.0","3.0","3.0","4.0","4.0"]
["","","","Max.","kW","15.0","20.0","24.0","28.0","15.0","20.0","24.0","28.0"]
["","Efficacité","","Caractéristiques NL (DIN4708)","","2.1","2.1","2.1","2.2","2.1","2.1","2.1","2.2"]
["Gaz de carneau","Température","","Max.","°C","63","69","64","68","63","69","64","68"]
["","Débit massique (G31)","","Max.","kg/h","22.5","30.0","35.7","41.0","22.5","30.0","35.7","41.0"]
["Air d'alimentation","Concentrique","","","","Oui","Oui","Oui","Oui","Oui","Oui","Oui","Oui"]
["Production d'eau chaude sanitaire","Général","","Classe","","A","A","A","A","A","A","A","A"]
["","","","Profil de charge déclaré","","XL","XL","XL","XL","XL","XL","XL","XL"]
["Dimensions","Unité","Hauteur","Caisson","mm","1,895","1,895","1,895","1,895","1,895","1,895","1,895","1,895"]
["Caisson","Couleur","","","","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)"]
["Ballon","Matériau","","","","Polypropylène","Polypropylène","Polypropylène","Polypropylène","Polypropylène","Polypropylène","Polypropylène","Polypropylène"]
["Chauffage des locaux","Général","","Classe d'efficacité saisonnière du chauffage de l'air ambiant","","A","A","A","A","A","A","A","A"]
["","","","ηs (efficacité saisonnière du chauffage de l'air ambiant)","%","91","92","92","92","91","92","92","92"]
["Chauff. central","Apport de chaleur Qn (valeur calorifique brute)","Nom.","Min.","kW","3.3","3.3","4.4","4.4","3.3","3.3","4.4","4.4"]
["","","","Max.","kW","16.7","22.2","26.6","31.1","16.7","22.2","26.6","31.1"]
["","Température de l'eau","","Max.","°C","85","85","85","85","90","90","90","90"]
["","Sortie Pn à 80/60°C","","Min.","kW","2.9","2.9","3.9","3.9","2.9","2.9","3.9","3.9"]
["","","","Nom.","kW","14.6","19.5","23.4","27.2","14.6","19.5","23.4","27.2"]
["","Apport de chaleur Qn (valeur calorifique nette)","Nom.","Max.","kW","15.0","20.0","24.0","28.0","15.0","20.0","24.0","28.0"]
["","","","Min.","kW","3.0","3.0","4.0","4.0","3.0","3.0","4.0","4.0"]
["","Sortie Pnc à 50/30°C","","Min.","kW","3.2","3.2","4.3","4.3","3.2","3.2","4.3","4.3"]
["","","","Nom.","kW","15.7","20.9","25.0","29.1","15.7","20.9","25.0","29.1"]
["Gaz","Connexion","","Diamètre","mm","20","20","20","20","20","20","20","20"]
["","Consommation (G31)","","Min.","m³/h","0.16","0.16","0.27","0.27","0.16","0.16","0.27","0.27"]
["","","","Max.","m³/h","0.62","0.82","0.98","1.15","0.62","0.82","0.98","1.15"]
["","Catégorie NOx","","","","6","6","6","6","6","6","6","6"]
["Remarques","","","","","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897"]