{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DucoBox Energy Comfort"]
[]
[]
[]
[]
["","","","","","DucoBox Energy Comfort 325","DucoBox Energy Comfort D400"]
["Numéro d’article","","","","","00004485","00004707"]
["Puissance absorbée - 50&nbsp;Hz","Puissance absorbée - 50&nbsp;Hz-=-Mode échange de chaleur","Puissance absorbée - 50&nbsp;Hz-=-Mode échange de chaleur-=-Nom.","Puissance absorbée - 50&nbsp;Hz-=-Mode échange de chaleur-=-Nom.-=-Très élevé-=-kW","kW","0.131 (1)"]
["","Puissance absorbée - 50&nbsp;Hz-=-Mode dérivation","Puissance absorbée - 50&nbsp;Hz-=-Mode dérivation-=-Nom.","Puissance absorbée - 50&nbsp;Hz-=-Mode dérivation-=-Nom.-=-Très élevé-=-kW","kW","0.131 (1)"]
["Caisson","Matériau","","","","Tôle d’acier enduite + EPP","Tôle d’acier enduite + EPP"]
["Dimensions","Unité","","Hauteur","mm","705","800"]
["","","","Largeur","mm","700","756"]
["","","","Profondeur","mm","525","583"]
["Poids","Unité","","","kg","21","47"]
["Ventilateur","Ventilateur-=-Débit d'air - 50&nbsp;Hz","Ventilateur-=-Débit d'air - 50&nbsp;Hz-=-Mode échange de chaleur","Ventilateur-=-Débit d'air - 50&nbsp;Hz-=-Mode échange de chaleur-=-Très élevé-=-m³/h","m³/h","325","400"]
["","","Ventilateur-=-Débit d'air - 50&nbsp;Hz-=-Mode dérivation","Ventilateur-=-Débit d'air - 50&nbsp;Hz-=-Mode dérivation-=-Très élevé-=-m³/h","m³/h","325","400"]
["","Ventilateur-=-Pression statique extérieure - 50&nbsp;Hz","","Ventilateur-=-Pression statique extérieure - 50&nbsp;Hz-=-Très élevé-=-Pa","Pa","100"]
["Plage de fonctionnement","Autour de l'unité","","","°CBS","-5°C~40°CBS, 90 % HR ou moins"]
["Niveau de pression sonore - 50Hz","Mode échange de chaleur","","Très élevé","dBA","63"]
["","Mode dérivation","","Très élevé","dBA","63"]
["Système d'échange de chaleur","","","","","Air au courant transversal Echange chaleur totale (Chaleur sensible+chaleur latente)","Air au courant transversal Echange chaleur totale (Chaleur sensible+chaleur latente)"]
["Éléments d'échange de chaleur","","","","","PET/Polystyrène","v1 : PP - v2 : PET/Alu"]
["Diamètre de gaine de raccordement","mm","","","","Diamètre interne Ø160","180"]
["Mode de fonctionnement","","","","","Mode chauffage, Mode dérivation, Mode protection antigel","Mode chauffage, Mode dérivation, Mode protection antigel"]
["Classe CSE","","","","","A+","Voir remarque 2"]
["Débit maximum avec une PSE de 100 Pa","Débit","","","m³/h","325","400"]
["Niveau de puissance sonore (Lwa)","dB","","","","55","55"]
["Consommation électrique annuelle","kWh/a","","","","117.3","231.7 (1)"]
["Économies annuelles en Chauffage","Climat moyen","","","kWh/a","4714","4515 (1)"]
["","Climat froid","","","kWh/a","9222","8833 (1)"]
["","Climat chaud","","","kWh/a","2132","2042 (1)"]
["Alimentation électrique","Phase","","","","Monophasé mis à la terre","3-core power cable with earthed plug"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","230","230"]
["Remarques","","","","","(1) - À débit max.","(1) - Commande manuelle (sans DCV)"]
["","","","","","(2) - À 250 m3/h","(2) - Avec 2 capteurs (facteur de contrôle 0,65) : A+ ; Autres : A"]
["","","","","","(3) - À 100 m3/h","(3) - Filtre dynamique air soufflé (520 x 190 x 15 mm) Standard : ISO 16890 gros grains 65% (= G4) En option : ISO 16890 ePM1 55% (=F7) Filtre dynamique air évacué (520 x 190 x 15 mm) Standard : ISO 16890 gros grains 65% (= G4)"]
["","","","","","(4) - À 325 m3/h"]
["","","","","","(5) - À 332 m3/h"]
["","","","","","(6) - À 401 m3/h"]