{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","E1500"]
[]
[]
[]
[]
["","","","","EZESHP20AUAW1B"]
["Puissance frigorifique","À un point de consigne de 0 °C (température ambiante de 30 °C)","R-452A","kW","14,900"]
["","À un point de consigne de -20 °C (température ambiante de 30 °C)","R-452A","kW","9,200"]
["Puissance calorifique","À un point de consigne de +2 °C (température ambiante de -20 °C)","R-452A","kW","10,500"]
["Puissance absorbée","Moteur","Type","","Kubota Custom Diesel Engine, 4 Cylinders, NRMM Stage V Compliant"]
["","","Déplacement","cc","1,500"]
["","","Fréquence de la maintenance","Temps de montée en température de 10°C à 50°C","3,000"]
["","Générateur","Type","","Direct Drive"]
["","","Alim.","kW","15"]
["Dimensions","Unité","Hauteur","mm","2,227"]
["","","Largeur","mm","2,072"]
["","","Profondeur","mm","440"]
["","Unité emballée","Hauteur","mm","2,066"]
["","","Largeur","mm","2,345"]
["","","Profondeur","mm","542"]
["Poids","Unité","","kg","730"]
["Compresseur","Type","","","Custom Scroll Compressor - Economizer/Inverter"]
["Réfrigérant","Type","","","R-452A"]
["Niveau de pression sonore","Nom.","","dBA","65"]
["Power supply","Tension","","V","400"]
["","Phase","","","3P+N"]
["","Fréquence","","Hz","50"]