{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":10,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EAVH-D9WG / EPGA011-016DV"]
[]
[]
[]
[]
["","","","","EAVH16S18DA9WG / EPGA11DAV3","EAVH16S23DA9WG / EPGA11DAV3","EAVH16S18DA9WG / EPGA14DAV3","EAVH16S23DA9WG / EPGA14DAV3","EAVH16S18DA9WG / EPGA16DAV3","EAVH16S23DA9WG / EPGA16DAV3"]
["Chauffage d'eau chaude sanitaire","Général","Profil de charge déclaré","","L","XL","L","XL","L","XL"]
["","Climat moyen","Classe","","A","A","A","A","A","A"]
["COP","","","","5.15 (1), 3.88 (2)","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)","4.78 (1), 3.71 (2)"]
["Unité intérieure","","","","EAVH16S18DA9W","EAVH16S23DA9W","EAVH16S18DA9W","EAVH16S23DA9W","EAVH16S18DA9W","EAVH16S23DA9W"]
["Puissance calorifique","Nom.","","kW","11.1 (1), 11.3 (2)","11.1 (1), 11.3 (2)","14.5 (1), 14.5 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)","16.5 (1), 15.6 (2)"]
["Puissance absorbée","Chauffage","Nom.","kW","2.16 (1), 2.91 (2)","2.16 (1), 2.91 (2)","2.91 (1), 3.96 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)","3.45 (1), 4.21 (2)"]
["Remarques","","","","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)"]