{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAH-D9W"]
[]
[]
[]
[]
["","","","","","EGSAH06DA9W","EGSAH10DA9W"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","","kW","0.85","0.85"]
["","Nom.","","","kW","3.35","5.49"]
["","Max.","","","kW","7.98","9.55"]
["Puissance absorbée","Nom.","","","kW","0.74","1.17"]
["COP","","","","","4.51","4.7"]
["Caisson","Couleur","","","","Blanc + noir","Blanc + noir"]
["","Matériau","","","","Tôle avec précouche"]
["Dimensions","Unité","","Hauteur","mm","1891","1891"]
["","","","Largeur","mm","597","597"]
["","","","Profondeur","mm","666","666"]
["Poids","Unité","","","kg","222","222"]
["Réservoir","Volume d'eau","","","L","180","180"]
["","Isolation","","Réservoir-=-Isolation-=-Perte thermique-=-kWh/24&nbsp;h","kWh/24 h","1.2","1.2"]
["","Protection contre la corrosion","","","","Décapage","Décapage"]
["Réfrigérant","Type","","","","R-32","R-32"]
["","Réfrigérant-=-PRP","","","","675.0","675.0"]
["","Charge","","","tCO2Eq","1.15","1.15"]
["","Charge","","","kg","1.70","1.70"]
["Chauffage des locaux","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-SCOP","","3.72 (1)","4.00 (1)"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A++","A+++"]
["","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-SCOP","","5.06 (1)","5.12 (1)"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A+++","A+++"]
["Alimentation électrique","Phase","","","","1~/3~","1~/3~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","230/400","230/400"]
["Courant","Fusibles recommandés","","","A","16/32","16/32"]
["Remarques","","","","","(1) - Conformément aux normes EN14825 et EN14511:2018","(1) - Conformément aux normes EN14825 et EN14511:2018"]