{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-E6V / ERGA-EV"]
[]
[]
[]
[]
["","","","","","EHBH04EA6V / ERGA04EAV3","EHBH04EF6V / ERGA04EAV3"]
["Puissance calorifique","Nom.","","","kW","4.3 (1), 4.6 (2)","4.3 (1), 4.6 (2)"]
["Puissance absorbée","Chauffage","","Nom.","kW","0.85 (1), 1.26 (2)","0.85 (1), 1.26 (2)"]
["COP","","","","","5.1 (1), 3.65 (2)","5.1 (1), 3.65 (2)"]
["Chauffage des locaux","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-SCOP","","3.26","3.26"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A++","A++"]
["","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-SCOP","","4.48","4.48"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A+++","A+++"]
["Remarques","","","","","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2 : rafraîchissement Ta 35°C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 45 °C (DT = 5°C)","(2) - Condition 2 : rafraîchissement Ta 35°C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 45 °C (DT = 5°C)"]