{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHFH-D3V / ERLA-DV"]
[]
[]
[]
[]
["","","","","EHFH03S18DA3V / ERLA03DAV3","EHFH03S18DJ3V / ERLA03DAV3"]
["Chauffage d'eau chaude sanitaire","Général","Profil de charge déclaré","","","L"]
["","Climat moyen","Classe","","","A"]
["COP","","","","4.91 (1), 2.95 (2)","5.00 (1), 2.94 (2)"]
["Puissance frigorifique","Nom.","","kW","","3.44 (1), 3.49 (2)"]
["","Min.","","kW","","1.8 (1)"]
["EER","","","","","5.60 (1), 3.03 (2)"]
["Puissance calorifique","Nom.","","kW","","3.59 (1), 3.53 (2)"]
["","Min.","","kW","","1.26 (1)"]
["Puissance absorbée","Rafraîchissement","Min.","kW","","0.62 (1), 1.17 (2)"]
["","Chauffage","Nom.","kW","","0.720 (1), 1.21 (2)"]
["Remarques","","","","(1) - Condition 1 : rafraîchissement Ta 35°C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","(2) - Condition 5 : Rafraîchissement Ta 35°C - LWE 7°C (DT = 5°C) ; Chauffage Ta BS/BH 7°C/6°C - LWC 55°C (DT = 8°C)","(2) - Condition 5 : Rafraîchissement Ta 35°C - LWE 7°C (DT = 5°C) ; Chauffage Ta BS/BH 7°C/6°C - LWC 55°C (DT = 8°C)"]
["","","","","","(3) - Rafraîchissement Ta 35 °C - LWE 18℃ (DT = 5 °C) ; chauffage Ta DB/WB 7 °C/6 °C - LWC 35℃ (DT = 5 °C)"]
["Puissance calorifique","Nom.","","kW","3.50 (2) (1)"]
["Puissance absorbée","Chauffage","Nom.","kW","0.710 (1), 1.19 (2)"]
["Chauffage d'eau chaude sanitaire","Général","Profil de charge déclaré","","L"]