{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHOBG-A"]
[]
[]
[]
[]
["","","","","","EHOBG12ABV1","EHOBG18ABV1","EHOBG12AAV1","EHOBG18AAV1"]
["Gaz de carneau","Température","","Max.","°C","","","","70"]
["","Débit massique (G31)","","Max.","kg/h","","","","30.6"]
["Air d'alimentation","Concentrique","","","","","","","60/100"]
["Dimensions","Unité","Hauteur","Caisson","mm","","","","590"]
["Casing","Material","","","","","","","Tôle avec précouche"]
["","Colour","","","","","","","RAL9010"]
["Chauffage des locaux","Général","","Classe d'efficacité saisonnière du chauffage de l'air ambiant","","","","","A"]
["","","","ηs (efficacité saisonnière du chauffage de l'air ambiant)","%","","","","92"]
["Chauff. central","Apport de chaleur Qn (valeur calorifique brute)","Nom.","Min.","kW","","","","6.2"]
["","","","Max.","kW","","","","20.8"]
["","Température de l'eau","","Max.","°C","","","","90"]
["","Sortie Pn à 80/60°C","","Nom.","kW","","","","18.2"]
["","Apport de chaleur Qn (valeur calorifique nette)","Nom.","Max.","kW","","","","18.7"]
["","","","Min.","kW","","","","5.6"]
["Gaz","Connexion","","Diamètre","mm","","","","15"]
["","Consommation (G31)","","Min.","m³/h","","","","0.22"]
["","","","Max.","m³/h","","","","0.74"]
["","Catégorie NOx","","","","","","","6"]
["Gaz","Connexion","","Diamètre","mm","15","15","15"]
["","Consommation (G20)","","Min.","m³/h","0.36","0.58","0.36"]
["","","","Max.","m³/h","1.30","1.94","1.30"]
["","Consommation (G25)","","Min.","m³/h","0.42","0.67","0.42"]
["","","","Max.","m³/h","1.50","2.25","1.50"]
["","Consommation (G31)","","Min.","m³/h","0.14","0.22","0.14"]
["","","","Max.","m³/h","0.49","0.74","0.49"]
["","Catégorie NOx","","","","6","6","6"]
["","Niveau NOx (G20)","","","mg/kWh","28","28","28"]
["Chauffage central","Apport de chaleur Qn (valeur calorifique nette)","Nom.","Min.","kW","3.8","5.6","3.8"]
["","","","Max.","kW","12.5","18.7","12.5"]
["","Apport de chaleur Qn (valeur calorifique brute)","Nom.","Min.","kW","4.2","6.2","4.2"]
["","","","Max.","kW","13.9","20.8","13.9"]
["","Chauffage central-=-Sortie Pn à 80/60 °C","","Chauffage central-=-Sortie Pn à 80/60 °C-=-Nom.-=-kW","kW","12.2","18.2","12.2"]
["","Chauffage central-=-Sortie à 37/30 °C","","Chauffage central-=-Sortie à 37/30 °C-=-Nom.-=-kW","kW","4.1","6.1","4.1"]
["","Température de l'eau","","Max.","°C","90","90","90"]
["Air d'alimentation","Concentrique","","","","non","non","non"]
["Gaz de carneau","Température","","Max.","°C","70","70","70"]
["","Connexion","","","mm","60","60","60"]
["","Débit massique (G20)","","Max.","kg/h","20.9","31.3","20.9"]
["","Débit massique (G25)","","Gaz de carneau-=-Débit massique (G25)-=-Max.-=-kg/h","kg/h","20.9","31.3","20.9"]
["","Débit massique (G31)","","Max.","kg/h","20.5","30.6","20.5"]
["Caisson","Couleur","","","","RAL9010","RAL9010","RAL9010"]
["","Matériau","","","","Tôle avec précouche","Tôle avec précouche","Tôle avec précouche"]
["Dimensions","Unité","Hauteur","Caisson","mm","590","590","590"]
["","","","Largeur","mm","450","450","450"]
["","","","Profondeur","mm","240","240","240"]
["Poids","Unité","","Vide","kg","30","30","30"]
["Chauffage de l'air ambiant","Général","","Classe d'efficacité saisonnière du chauffage de l'air ambiant","","A","A","A"]
["Classe d'efficacité énergétique","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]