{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3"]
[]
[]
[]
[]
["","","","","","EHSX04P30DA3","EHSX04P50DA3","EHSX08P30DA3","EHSX08P50DA3"]
["Caisson","Couleur","","","","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)"]
["","Matériau","","","","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc"]
["Dimensions","Unité","","Hauteur","mm","1891","1896","1891","1896"]
["","","","Largeur","mm","595","790","595","790"]
["","","","Profondeur","mm","615","790","615","790"]
["Poids","Unité","","","kg","73.0","93.0","73.0","93.0"]
["DESP","Catégorie","","","","art. 3,3","art. 3,3","art. 3,3","art. 3,3"]
["Réfrigérant","","","","","R-32","R-32","R-32","R-32"]
["","Réfrigérant-=-PRP","","","","675.0","675.0","675.0","675.0"]
["","Charge","","","kg","1.50","1.50","1.50","1.50"]
["Niveau de puissance sonore","Nom.","","","dBA","39","39","39","39"]
["Plage de fonctionnement","Chauffage","Côté eau","Min.","°C","18","18","18","18"]
["","","","Max.","°C","65","65","65","65"]
["","Rafraîchissement","Temp. ext.","Min.","°CBS","10","10","10","10"]
["","","Côté eau","Min.","°C","5","5","5","5"]
["","","","Max.","°C","22","22","22","22"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","230","230","230","230"]
["Dispositif de chauffage électrique","Alimentation électrique","","Nom","","3V / 9W","3V / 9W","3V / 9W","3V / 9W"]
["","","","Phase","","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Fréquence","Hz","50","50","50","50"]
["Remarques","","","","","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897"]
["","","","","","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C"]
["","","","","","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60 ℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60 ℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60 ℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60 ℃"]
["","","","","","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65 ℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65 ℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65 ℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65 ℃"]
["","","","","","","(5) - Chauff. du réserv. uniq. avec pompe à chal., pas de rad. élect.","","(5) - Chauff. du réserv. uniq. avec pompe à chal., pas de rad. élect."]