{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSXB-E"]
[]
[]
[]
[]
["","","","","","EHSXB04P30EG","EHSXB04P50EG","EHSXB08P30EG","EHSXB08P50EG","EHSXB04P30EF (Archived)","EHSXB04P50EF (Archived)","EHSXB08P30EF (Archived)","EHSXB08P50EF (Archived)"]
["Caisson","Couleur","","","","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)"]
["","Matériau","","","","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc"]
["Dimensions","Unité","","Hauteur","mm","1,891","1,910","1,891","1,910","1,892","1,905","1,892","1,905"]
["","","","Largeur","mm","594","792","594","792","594","792","594","792"]
["","","","Profondeur","mm","644","817","644","817","644","812","644","812"]
["Poids","Unité","","","kg","80.0","104","80.0","104","79","110","79","110"]
["DESP","Catégorie","","","","Art 4.3","Art 4.3","Art 4.3","Art 4.3","Art 4.3","Art 4.3","Art 4.3","Art 4.3"]
["Réfrigérant","","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Réfrigérant-=-PRP","","","","675.0","675.0","675.0","675.0","675","675","675","675"]
["","Charge","","","kg","1.50","1.50","1.50","1.50","1.5","1.5","1.5","1.5"]
["Niveau de puissance sonore","Nom.","","","dBA","39","39","39","39","39","39","39","39"]
["Plage de fonctionnement","Chauffage","Côté eau","Min.","°C","18","18","18","18","18","18","18","18"]
["","","","Max.","°C","65","65","65","65","65","65","65","65"]
["","Rafraîchissement","Temp. ext.","Min.","°CBS","10","10","10","10","10","10","10","10"]
["","","Côté eau","Min.","°C","5","5","5","5","5","5","5","5"]
["","","","Max.","°C","22","22","22","22","22","22","22","22"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","230","230","230","230","230","230","230","230"]
["Remarques","","","","","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897"]