{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E3V / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHVX04S23EJ3V / ERGA04EAV37","EHVX04S18EA3V / ERGA04EAV37","EHVX04S18EJ3V / ERGA04EAV37","EHVX04S23EA3V / ERGA04EAV37"]
["Puissance calorifique","Nom.","","","kW","4.36, 4.60","4.36, 4.60","4.36, 4.60","4.36, 4.60"]
["Puissance frigorifique","Nom.","","","kW","4.86, 4.52","4.86, 4.52","4.86, 4.52","4.86, 4.52"]
["Puissance absorbée","Chauffage","","Nom.","kW","0.830, 1.26","0.830, 1.26","0.830, 1.26","0.830, 1.26"]
["","Rafraîchissement","","Nom.","kW","0.810, 1.36","0.810, 1.36","0.810, 1.36","0.810, 1.36"]
["","Eau chaude sanitaire de 10°C à 50°C","","Nom.","kWh","3.01","2.48","2.48","3.01"]
["hr","Temps de montée en température de 10°C à 50°C","","","","1h40min","1h28min","1h28min","1h40min"]
["COP","","","","","5.23, 3.65","5.23, 3.65","5.23, 3.65","5.23, 3.65"]
["EER","","","","","5.98, 3.32","5.98, 3.32","5.98, 3.32","5.98, 3.32"]
["Chauffage d'eau chaude sanitaire","Général","","Profil de charge déclaré","","XL","L","L","XL"]
["","Climat moyen","","Classe","","A","A","A","A"]
["Chauffage des locaux","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-SCOP","","3.29","3.29","3.29","3.29"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A++","A++","A++","A++"]
["","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-SCOP","","4.96","4.96","4.96","4.96"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A+++","A+++","A+++","A+++"]
["Remarques","","","","","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)"]