{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHY2KOMB-A / EJHA-AV3"]
[]
[]
[]
[]
["","","","","","EHY2KOMB28AA / EJHA04AAV3","EHY2KOMB32AA / EJHA04AAV3"]
["Production d'eau chaude sanitaire","Général","","Profil de charge déclaré","","XL","XL"]
["","Climat moyen","","Classe","","A","A"]
["COP","","","","","4.49 (1)","4.49 (1)"]
["Pompe","PSE","Chauffage","Min.","kPa","25.0 (4)","25.0 (4)"]
["","","","Max","kPa","45.0 (4)","45.0 (4)"]
["Chauffage des locaux","Sortie d'eau sous climat tempéré 55 °C","Général","Seasonal space heating eff. class","","A++","A++"]
["","","","ηs (effic. saisonnière du chauffage d'ambiance)","%","128","128"]
["","","","SCOP","","3.26","3.28"]
["Puissance calorifique","Nom.","","","kW","3.83 (1)","3.83 (1)"]
["","Max.","","","kW","4.53 (1)","4.53 (1)"]
["Puissance absorbée","Chauffage","","Max.","kW","1.07 (1)","1.07 (1)"]
["","","","Nom.","kW","0.850 (1)","0.850 (1)"]
["Remarques","","","","","(1) - Chauffage : temp. de l'eau de sortie du condenseur 35℃ ; Dt 5°C ; temp. de l'air extérieur 7 °CBS, 6 °CBH","(1) - Chauffage : temp. de l'eau de sortie du condenseur 35℃ ; Dt 5°C ; temp. de l'air extérieur 7 °CBS, 6 °CBH"]
["","","","","","(2) - 7 °C/6 °C BS/BH - LWC 35 °C (DT=5 °C), dérivation de chaudière","(2) - 7 °C/6 °C BS/BH - LWC 35 °C (DT=5 °C), dérivation de chaudière"]
["","","","","","(3) - 7 °C/6 °C BS/BH - LWC 45 ℃ (DT=5 °C), dérivation de chaudière","(3) - 7 °C/6 °C BS/BH - LWC 45 ℃ (DT=5 °C), dérivation de chaudière"]
["","","","","","(4) - En fonction de la longueur de tuyauterie sur site","(4) - En fonction de la longueur de tuyauterie sur site"]