{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":7,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYKOMB-AA2"]
[]
[]
[]
[]
["","","","","","EHYKOMB33AA2","EHYKOMB33AA2A"]
["Gaz","Connexion","","Diamètre","mm","15","15"]
["","Consommation (G20)","","Min.","m³/h","0.79","0.79"]
["","","","Max.","m³/h","3.39","3.39"]
["","Consommation (G25)","","Min.","m³/h","0.89","0.89"]
["","","","Max.","m³/h","3.92","3.92"]
["","Consommation (G31)","","Min.","m³/h","0.30","0.30"]
["","","","Max.","m³/h","1.29","1.29"]
["","Catégorie NOx","","","","6","6"]
["","Niveau NOx (G20)","","","mg/kWh","36","36"]
["Chauffage central","Apport de chaleur Qn (valeur calorifique nette)","Nom.","Min.","kW","7.6","7.6"]
["","","","Max.","kW","27.0","27.0"]
["","Apport de chaleur Qn (valeur calorifique brute)","Nom.","Min.","kW","8.4","8.4"]
["","","","Max.","kW","30.0","30.0"]
["","Chauffage central-=-Sortie Pn à 80/60&nbsp;°C","","Chauffage central-=-Sortie Pn à 80/60&nbsp;°C-=-Min.-=-kW","kW","7.5","7.5"]
["","","","Chauffage central-=-Sortie Pn à 80/60&nbsp;°C-=-Nom.-=-kW","kW","26.6","26.6"]
["","Chauffage central-=-Sortie à 37/30&nbsp;°C","","Chauffage central-=-Sortie à 37/30&nbsp;°C-=-Nom.-=-kW","kW","8.2","8.2"]
["","Température de l'eau","","Max.","°C","90","90"]
["Eau chaude sanitaire","Apport de chaleur (valeur calorifique nette) Qnw","Nom.","Min.","kW","7.6","7.6"]
["","","","Max.","kW","32.7","32.7"]
["","Apport de chaleur (valeur calorifique brute) Qnw","Nom.","Min.","kW","8.4","8.4"]
["","","","Max.","kW","36.3","36.3"]
["","Classe de confort (EN13203)","","","","XL","XL"]
["","Température","","Max.","°C","65","65"]
["Air d'alimentation","Concentrique","","","","non","non"]
["Gaz de carneau","Température","","Max.","°C","70","70"]
["","Connexion","","","mm","60","60"]
["","Débit massique (G20)","","Max.","kg/h","54.4","54.4"]
["","Débit massique (G25)","","Gaz de carneau-=-Débit massique (G25)-=-Max.-=-kg/h","kg/h","54.4","54.4"]
["","Débit massique (G31)","","Max.","kg/h","53.6","53.6"]
["Caisson","Couleur","","","","RAL9010","RAL9010"]
["","Matériau","","","","Tôle avec précouche","Tôle avec précouche"]
["Dimensions","Unité","Hauteur","Caisson","mm","710","710"]
["","","","Largeur","mm","450","450"]
["","","","Profondeur","mm","240","240"]
["Poids","Unité","","Vide","kg","36","36"]
["Chauffage d'eau chaude sanitaire","Général","","Profil de charge déclaré","","XL","XL"]
["Production d'eau chaude sanitaire","Général","","Classe","","A","A"]
["Chauffage de l'air ambiant","Général","","Classe d'efficacité saisonnière du chauffage de l'air ambiant","","A","A"]