{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EJHA-AV3"]
[]
[]
[]
[]
["","","","","","EJHA04AAV3"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","37.0"]
["Réfrigérant","PRP","","","","675.0"]
["","Charge","","","kg","0.560"]
["","Type","","","","R-32"]
["Plage de fonctionnement","Chauffage","Extérieure","Max.","°CBH","25"]
["","Eau chaude sanitaire","Temp. ext.","Min.","°CBS","-14"]
["","","","Max.","°CBS","35"]
["Puissance absorbée","Chauffage","","Nom.","kW","0.850 (1)"]
["Niveau de puissance sonore","Chauffage","","Nom.","dBA","58.7"]
["COP","","","","","4.49 (1)"]
["Dimensions","Unité","","Largeur","mm","845"]
["","","","Profondeur","mm","329"]
["","","","Hauteur","mm","745"]
["Poids","Unité","","","kg","45.0"]
["Chauffage des locaux","Sortie d'eau climat tempéré35 °C","Général","ηs (effic. saisonnière du chauffage d'ambiance)","%","116"]
["","","","Classe d'effic. saisonnière du chauffage d'ambiance","","A"]
["","","","SCOP","","2.98"]
["","Sortie d'eau sous climat tempéré 55 °C","Général","Seasonal space heating eff. class","","A+"]
["","","","ηs (effic. saisonnière du chauffage d'ambiance)","%","101"]
["","","","SCOP","","2.60"]
["Ventil.","Débit d'air","Chauffage","Haut","m³/min","28.3"]
["Puissance calorifique","Nom.","","","kW","4.53 (1)"]
["Power supply","Phase","","","","1~"]
["","Nom","","","","V3"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","220-240"]
["Remarques","","","","","(1) - Chauffage : temp. de l'eau de sortie du condenseur 35℃ ; Dt 5°C ; temp. de l'air extérieur 7 °CBS, 6 °CBH"]