{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":7,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHH2E-AV3"]
[]
[]
[]
[]
["","","","","","EKHH2E200AAV3","EKHH2E260AAV3"]
["Sound power level","Production eau chaude sanitaire","","Unité intérieure","dBA","53","53"]
["","","","Outdoor unit","dBA","52","52"]
["Chauffage d'eau chaude sanitaire","Général","","Classe","","A+","A+"]
["","","","Réglage temp. thermostat","°C","55","55"]
["","","","Profil de charge déclaré","","L","XL"]
["","Climat froid","","AEC (consommation électrique annuelle)","kWh","1,091","1,826"]
["","Climat chaud","","AEC (consommation électrique annuelle)","kWh","756","1,296"]
["","Climat moyen","","AEC (consommation électrique annuelle)","kWh","835","1,323"]
["Équivalent eau chaude","Max.","","","L","275","342"]
["Pompe à chaleur","Automatic defrost start","","","°C","-2","-2"]
["","Plage de fonctionnement","Temp. ext.","Min.","°CBS","-7","-7"]
["","","","Max.","°CBS","38","38"]
["","Casing","","Material","","Couvercle : Finition supérieure EPP","Couvercle : Finition supérieure EPP"]
["","","","Couleur","","White body / black top","White body / black top"]
["","Pression du circuit","","Max.","bars","7","7"]
["","Méthode de dégivrage","","","","Actif avec vanne gaz chauds","Actif avec vanne gaz chauds"]
["COP","","","","","2.94 (1), 3.30 (2)","3.10 (1), 3.60 (2)"]
["Réfrigérant","PRP","","","","1,430.0","1,430.0"]
["","Charge","","","kg","0.900","0.900"]
["","Type","","","","R-134a","R-134a"]
["Compresseur","Type","","","","Rotary non-inverter","Rotary non-inverter"]
["Dimensions","Unité","","Diamètre","mm","650","650"]
["","","","Hauteur","mm","1,714","2,000"]
["Eau chaude sanitaire","Sortie","","Nom.","kW","1.8","1.8"]
["Réservoir","Installation","","Possibilité de raccordement héliothermique","","Non","Non"]
["","Puissance de l’élément de chauffage intégré","","Nom.","kW","1.5","1.5"]
["","Caisson","","Matériau","","ABS gaufré","ABS gaufré"]
["","","","Couleur","","Blanc","Blanc"]
["","Dimensions","Unité","Hauteur","mm","1,210","1,500"]
["","Plage de fonctionnement","Côté eau","Max.","°C","56","56"]
["","","","Min.","°C","10","10"]
["Poids","Unité emballée","","","kg","103","115"]
["","Unité","","Vide","kg","83","95"]
["","","","Pleine","kg","282","349"]
["Lieu d'installation","","","","","Intérieur","Intérieur"]
["IP class","","","","","IP-X4","IP-X4"]
["Général","Description du produit","","Pompe à chaleur air-eau","","Oui","Oui"]
["","Coordonnées du fournisseur/fabricant","","Nom et adresse","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Temps de montée en température","Max.","","","hh:mm","08:17:00, 06:30:44","10:14:00, 07:56:46"]
["Pompe à chaleur","Alimentation électrique","","Fréquence","Hz","50","50"]
["","","","Courant de fonctionnement maximum","A","2","2"]
["","","","Phase","","1P","1P"]
["","","","Tension","V","230","230"]
["Réservoir","Alimentation électrique","","Phase","","1P","1P"]
["","","","Fréquence","Hz","50","50"]
["","","","Tension","V","230","230"]
["Remarques","","","","","(1) - Selon la norme EN16147-2011, température à l'entrée 7 °C, température ambiante 20 °C, admission d'eau froide 10 °C","(1) - Selon la norme EN16147-2011, température à l'entrée 7 °C, température ambiante 20 °C, admission d'eau froide 10 °C"]
["","","","","","(2) - Selon la norme EN16147-2011, température à l'entrée 15 °C, température ambiante 20 °C, admission d'eau froide 10 °C","(2) - Selon la norme EN16147-2011, température à l'entrée 15 °C, température ambiante 20 °C, admission d'eau froide 10 °C"]
["","","","","","(3) - Température intérieure : 29 °CBS, 19 °CBH ; température extérieure : 46 ° CBS, 24 ° CBH","(3) - Température intérieure : 29 °CBS, 19 °CBH ; température extérieure : 46 ° CBS, 24 ° CBH"]
["","","","","","(4) - Température intérieure : 27 ° CBS, 19 ° CBH ; température extérieure : 35 ° CBS, 24 ° CBH","(4) - Température intérieure : 27 ° CBS, 19 ° CBH ; température extérieure : 35 ° CBS, 24 ° CBH"]