{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":77,"n_cols":7,"rows_kept":77,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHHE-CV37"]
[]
[]
[]
[]
["","","","","","EKHHE200CV37","EKHHE260CV37"]
["Temps de montée en température","Max.","","","hh:mm","06:27:00","09:29:00"]
["COP","","","","","3.23","3.37"]
["Eau chaude sanitaire","Sortie","","Nom.","kW","1.339","1249"]
["Équivalent eau chaude","Max.","","","L","247","340"]
["Dimensions","Unité","","Hauteur","mm","1607","1892"]
["","","","Diamètre","mm","621","621"]
["Poids","Unité","","Vide","kg","85","97"]
["","","","Pleine","kg","277","347"]
["Dimensions","Unité","Hauteur","Intégré sur l'unité intérieure","mm","1607","1892"]
["Poids","Unité emballée","","","kg","96","109"]
["Lieu d'installation","","","","","Intérieur","Intérieur"]
["Classe IP","","","","","IP24","IP24"]
["Compresseur","Type","","","","Rotatif","Rotatif"]
["Réfrigérant","","","","","R-134a","R-134a"]
["Pompe à chaleur","Nom","","","","EKHHE200CV37","EKHHE260CV37"]
["Réfrigérant","Réfrigérant-=-PRP","","","","1430","1430"]
["","Réfrigérant-=-Charge-=-Téq. CO₂","","","Téq. CO₂","1.43","1.43"]
["","Charge","","","kg","1","1"]
["Pompe à chaleur","Puissance calorifique","","","kW","0.43","0.43"]
["","Caisson","","Couleur","","Blanc","Blanc"]
["","Dimensions","Unité","Hauteur","mm","1607","1892"]
["","","","Largeur","mm","621","621"]
["","","","Profondeur","mm","621","621"]
["","Poids","","Unité","kg","85","97"]
["","","","Unité à garniture","kg","96","109"]
["","Lieu d'installation","","","","Intérieur seulement","Intérieur seulement"]
["","Installation","","Classe IP","","IP24","IP24"]
["","","","Distance par rapport au mur","mm","200","200"]
["","Plage de fonctionnement","Temp. ext.","Min.","°CBS","-7","-7"]
["","","","Max.","°CBS","43","43"]
["","Niveau de pression sonore","","Nom.","dBA","53","51"]
["","","","Mode nuit","dBA","53.0","51"]
["","Réfrigérant","","Pompe à chaleur-=-Réfrigérant-=-Type","","R-134A","R-134A"]
["","","","PRP","","1430","1430"]
["","","","Pompe à chaleur-=-Réfrigérant-=-Charge-=-Téq. CO₂","Téq. CO₂","1.43","1.43"]
["","","","Charge","kg","1","1"]
["","Méthode de dégivrage","","","","Dégivrage par gaz chaud","Dégivrage par gaz chaud"]
["","Pression du circuit","","Max.","bars","7","7"]
["Réservoir","Puissance de l’élément de chauffage intégré","","Nom.","kW","1.5","1.5"]
["","Caisson","","Couleur","","Blanc","Blanc"]
["","","","Matériau","","Acier émaillé","Acier émaillé"]
["","Lieu d'installation","","","","Intérieur seulement","Intérieur seulement"]
["","Installation","","Classe IP","","IP24","IP24"]
["","","","Possibilité de raccordement héliothermique","","Non","Non"]
["","","","Orifice de recyclage du réservoir","","Non","Non"]
["Général","Description du produit","","Pompe à chaleur air-eau","","Oui","Oui"]
["","","","Identification du modèle","","EKHHE200CV37","EKHHE260CV37"]
["","Appareil de chauffage supplémentaire","","Type d'apport en énergie","","Électricité","Électricité"]
["","Coordonnées du fournisseur/fabricant","","Nom ou marque de commerce","","Daikin Europe N.V.","Daikin Europe N.V."]
["","Niveau de puissance acoustique LW(A) (conformément à la norme EN14825)","","Général-=-Niveau de puissance acoustique LW(A) (conformément à la norme EN14825)-=-Intérieur-=-dBA","dBA","53","51"]
["Chauffage d'eau chaude sanitaire","Général","","Profil de charge déclaré","","L","XL"]
["","","","Fonction pour régler le chauffage de l'eau en dehors des heures de pic","","Oui","Oui"]
["Production d'eau chaude sanitaire","Général","","Classe","","A+","A+"]
["Production eau chaude sanitaire","Général","","Réglage temp. thermostat","°C","55","55"]
["Niveau puiss. sonore","Production eau chaude sanitaire","","Unité extérieure","dBA","45","44"]
["","","","Unité intérieure","dBA","53","51"]
["Chauffage d'eau chaude sanitaire","Climat moyen","","AEC (consommation électrique annuelle)","kWh","761","1210"]
["","","","Qelec (consommation électrique quotidienne)","kWh","2.08","3.31"]
["","Climat froid","","AEC (consommation électrique annuelle)","kWh","944","1496"]
["","","","Qelec (consommation électrique quotidienne)","kWh","2.59","4.10"]
["","Climat chaud","","AEC (consommation électrique annuelle)","kWh","631","1046"]
["","","","Qelec (consommation électrique quotidienne)","kWh","1.73","2.87"]
["Classe d'efficacité énergétique","","","","","A+ ~ F","A+ ~ F"]
["Pompe à chaleur","Alimentation électrique","","Phase","","1P","1P"]
["","","","Fréquence","Hz","50","50"]
["","","","Tension","V","230","230"]
["","","","Courant de fonctionnement maximum","A","8.5","8.5"]
["","","","Utilisation sur site recommandée","A","2.43","2.43"]
["Réservoir","Alimentation électrique","","Phase","","1P","1P"]
["","","","Fréquence","Hz","50","50"]
["","","","Tension","V","230","230"]