{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":8,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWP-B"]
[]
[]
[]
[]
["","","","","","EKHWP300B","EKHWP54419BA","EKHWP500B"]
["Échangeur de chaleur","Eau chaude sanitaire","","Matériau du tuyau","","","Acier inoxydable (DIN 1,4404)"]
["","","","Pression de service","bars","","10.0"]
["","","","Volume interne de serpentin","L","","28.9"]
["","","","Quantité","","","1"]
["","Charge","","Quantité","","","1"]
["","","","Matériau du tuyau","","","Acier inoxydable (DIN 1,4404)"]
["","","","Pression de service","bars","","3.0"]
["","","","Volume interne de serpentin","L","","10.0"]
["","Chauffage solaire auxiliaire","","Volume interne de serpentin","L","","3.9"]
["","","","Matériau du tuyau","","","Acier inoxydable (DIN 1,4404)"]
["","","","Pression de service","bars","","3.0"]
["","","","Quantité","","","1"]
["Dimensions","Unité","","Largeur","mm","","790"]
["","","Hauteur","Ballon","mm","","1,658"]
["","","","Profondeur","mm","","790"]
["Caisson","Matériau","","","","","Polypropylène anti-choc"]
["","Couleur","","","","","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)"]
["Réservoir","Étiquette énergie","","","","","B"]
["","Température d'eau maximum","","","°C","","85"]
["","Matériau","","","","","Polypropylène"]
["","Volume d'eau","","","L","","477"]
["Poids","Unité","","Vide","kg","","71"]
["","","","Pleine","kg","","548"]
["Montage","","","","","","Sol"]
["Remarques","","","","","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897"]
["","","","","","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C"]
["","","","","","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60 ℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60 ℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60 ℃"]
["","","","","","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65 ℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65 ℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65 ℃"]
["","","","","","(5) - Pour volume de pompage de 140 l -> 5 820 Wh (bain) / pompe à chaleur 8 kW","(5) - Pour volume de pompage de 140 l -> 5 820 Wh (bain) / pompe à chaleur 8 kW","(5) - Pour volume de pompage de 140 l -> 5 820 Wh (bain) / pompe à chaleur 16 kW"]
["","","","","","(6) - Pour volume de pompage de 90 l -> 3 660 Wh (bain) / pompe à chaleur 8 kW","(6) - Pour volume de pompage de 90 l -> 3 660 Wh (bain) / pompe à chaleur 8 kW","(6) - Pour volume de pompage de 90 l -> 3 660 Wh (bain) / pompe à chaleur 16 kW"]
["","","","","","","(7) - Pour volume de pompage de 140 l -> 5 820 Wh (bain) / pompe à chaleur 16 kW"]
["","","","","","","(8) - Pour volume de pompage de 90 l -> 3 660 Wh (bain) / pompe à chaleur 16 kW"]
["","","","","","","(9) - Échangeur de chaleur raccordé en parallèle, TKW = 10°C / TWW = 45°C / TSP = 65°C / Pcharge = 35 kW / Tdébit = 80°C"]
["","","","","","","(10) - TKW = 10°C / TWW = 45°C / TSP = 65°C / Pcharge = 35 kW / Tdébit = 80°C"]
["Montage","","","","","Sol","","Sol"]
["Caisson","Couleur","","","","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)"]
["","Matériau","","","","Polypropylène anti-choc","","Polypropylène anti-choc"]
["Dimensions","Unité","Hauteur","Ballon","mm","1646","","1658"]
["","","","Largeur","mm","595","","790"]
["","","","Profondeur","mm","615","","790"]
["Poids","Unité","","Vide","kg","53","","76"]
["","","","Pleine","kg","347","","553"]
["Réservoir","Volume d'eau","","","L","294","","477"]
["","Matériau","","","","Polypropylène","","Polypropylène"]
["Ballon","Température d'eau maximum","","","°C","85","","85"]
["Réservoir","Étiquette énergie","","","","B","","B"]
["Échangeur de chaleur","Eau chaude sanitaire","","Quantité","","1","","1"]
["","","","Matériau du tuyau","","Acier inoxydable (DIN 1.4404)","","Acier inoxydable (DIN 1.4404)"]
["","","","Volume interne de serpentin","L","27.8","","28.9"]
["","","","Pression de service","bars","10.0","","10.0"]
["","Charge","","Quantité","","1","","1"]
["","","","Matériau du tuyau","","Acier inoxydable (DIN 1.4404)","","Acier inoxydable (DIN 1.4404)"]
["","","","Volume interne de serpentin","L","12.9","","18.1"]
["","","","Pression de service","bars","6.0","","6.0"]
["Échangeur de chaleur","Chauffage solaire auxiliaire","","Quantité","","","","1"]
["Échangeur de chaleur","Chauffage solaire auxiliaire","","Matériau du tuyau","","","","Acier inoxydable (DIN 1.4404)"]
["","","","Volume interne de serpentin","L","","","3.9"]
["Échangeur de chaleur","Chauffage solaire auxiliaire","","Pression de service","bars","","","3.0"]