{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWS-D3V3"]
[]
[]
[]
[]
["","","","","","EKHWS150D3V3","EKHWS180D3V3","EKHWS200D3V3","EKHWS250D3V3","EKHWS300D3V3"]
["Caisson","Couleur","","","","Blanc neutre","Blanc neutre","Blanc neutre","Blanc neutre","Blanc neutre"]
["","Matériau","","","","Acier revêtu d’époxy, Acier doux revêtu de résine époxy","Acier revêtu d’époxy, Acier doux revêtu de résine époxy","Acier revêtu d’époxy, Acier doux revêtu de résine époxy","Acier revêtu d’époxy, Acier doux revêtu de résine époxy","Acier revêtu d’époxy, Acier doux revêtu de résine époxy"]
["Dimensions","Unité","Hauteur","Ballon","mm","1,000","1,164","1,264","1,535","1,745"]
["","","","Diamètre","mm","595","595","595","595","595"]
["Poids","Unité","","Vide","kg","45","50","53","58","63"]
["","","","Pleine","kg","190","224","245","300","355"]
["Réservoir","Volume d'eau","","","L","145","174","192","242","292"]
["","Matériau","","","","Acier inoxydable (EN 1.4521)","Acier inoxydable (EN 1.4521)","Acier inoxydable (EN 1.4521)","Acier inoxydable (EN 1.4521)","Acier inoxydable (EN 1.4521)"]
["","Température d'eau maximum","","","°C","75","75","75","75","75"]
["","Étiquette énergie","","","","B","B","B","B","B"]
["Échangeur de chaleur","Eau chaude sanitaire","","Quantité","","1","1","1","1","1"]
["","","","Matériau du tuyau","","Acier inoxydable (EN 1.4521)","Acier inoxydable (EN 1.4521)","Acier inoxydable (EN 1.4521)","Acier inoxydable (EN 1.4521)","Acier inoxydable (EN 1.4521)"]
["","","","Volume interne de serpentin","L","4.9","6.5","8.2","8.2","8.2"]
["","","","Pression de service","bars","10","10","10","10","10"]
["Dispositif de chauffage d'appoint","Puissance","","","kW","3","3","3","3","3"]
["Remarques","","","","","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897"]