{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSV-P"]
[]
[]
[]
[]
["","","","","EKSV21P","EKSV21P1","EKSV26P","EKSV26P1"]
["Absorbeur","","","","Registre à tubes en cuivre en forme de harpe avec plaque d'aluminium soudée au laser et à revêtement hautement sélectif","Registre à tubes en cuivre en forme de harpe avec plaque d'aluminium soudée au laser et à revêtement hautement sélectif","Registre à tubes en cuivre en forme de harpe avec plaque d'aluminium soudée au laser et à revêtement hautement sélectif","Registre à tubes en cuivre en forme de harpe avec plaque d'aluminium soudée au laser et à revêtement hautement sélectif"]
["Température à l'arrêt","Max.","","°C","192","192","192","192"]
["Dimensions","Unité","Largeur","mm","85","1,006","85","1,300"]
["","","Profondeur","mm","2,000","85","2,000","85"]
["","","Hauteur","mm","1,006","2,000","1,300","2,000"]
["Pression de service","Max.","","bars","6","6","6","6"]
["Poids","Unité","","kg","33","35","42","42"]
["Surface","Ouverture","","m²","1.800","1.800","2.360","2.360"]
["","Absorbeur","","m²","1.79","1.80","2.35","2.36"]
["","Extérieure","","m²","2.01","2.01","2.60","2.60"]
["Montage","","","","Vertical","Vertical","Vertical","Vertical"]
["Couverture transparente","","","","Verre Sécurit, transmission + / - 92 %","Verre Sécurit, transmission + / - 92 %","Verre Sécurit, transmission + / - 92 %","Verre Sécurit, transmission + / - 92 %"]
["Angle de toiture autorisé","Max.","","°","80","80","80","80"]
["","Min.","","°","15","15","15","15"]
["Revêtement","","","","Microtherm (absorption max. 96%, Emission env. 5% +/-2%)","Microtherm (absorption max. 96%, Emission env. 5% +/-2%)","Microtherm (absorption max. 96%, Emission env. 5% +/-2%)","Microtherm (absorption max. 96%, Emission env. 5% +/-2%)"]
["Volume","L","","","1.3","1.3","1.7","1.7"]
["Performances thermiques","Efficacité perte nulle de collecteur η0","","%","0.781","0.710","0.784","0.710"]
["","Coefficient de perte thermique a1","","W/m².K²","4.240","4.300","4.250","4.300"]
["","Température liée au coefficient de perte thermique a2","","W/m².K²","0.006","0.006","0.007","0.006"]
["","Puissance calorifique","","kJ/K","4.9","4.9","6.5","6.5"]