{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSHB-E"]
[]
[]
[]
[]
["","","","","","ELSHB12P30EG","ELSHB12P50EG","ELSHB12P50EF (Archived)","ELSHB12P30EF (Archived)"]
["Caisson","Couleur","","","","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)","Blanc signalisation (RAL9016) / Noir signalisation (RAL9017)"]
["","Matériau","","","","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc","Polypropylène anti-choc"]
["Dimensions","Unité","","Hauteur","mm","1891","1910","1910","1893"]
["","","","Largeur","mm","594","792","792","594"]
["","","","Profondeur","mm","680","817","817","680"]
["Poids","Unité","","","kg","93.0","115","91.0","76.0"]
["DESP","Catégorie","","","","Catégorie II","Catégorie II","Catégorie II","Catégorie II"]
["Réfrigérant","","","","","R-32","R-32","R-32","R-32"]
["Niveau de puissance sonore","Nom.","","","dBA","44.7","44.7","44.7","44.7"]
["Niveau de pression sonore","Nom.","","","dBA","36.8","36.8","36.8","36.8"]
["Plage de fonctionnement","Chauffage","Côté eau","Min.","°C","15 (3)","15 (3)","15 (3)","15 (3)"]
["","","","Max.","°C","65 (3)","65 (3)","65 (3)","65 (3)"]
["","Rafraîchissement","Temp. ext.","Min.","°CBS","10 (3)","10 (3)","10 (3)","10 (3)"]
["","","Côté eau","Min.","°C","5 (3)","5 (3)","5 (3)","5 (3)"]
["","","","Max.","°C","22 (3)","22 (3)","22 (3)","22 (3)"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","230","230","230","230"]
["Remarques","","","","","(1) - La zone de fonctionnement est étendue aux débits inférieurs en fonction du mode de fonctionnement- se reporter à la courbe ESP.","(1) - La zone de fonctionnement est étendue aux débits inférieurs en fonction du mode de fonctionnement- se reporter à la courbe ESP.","(1) - La zone de fonctionnement est étendue aux débits inférieurs en fonction du mode de fonctionnement- se reporter à la courbe ESP.","(1) - La zone de fonctionnement est étendue aux débits inférieurs en fonction du mode de fonctionnement- se reporter à la courbe ESP."]
["","","","","","(2) - Perte de chaleur conforme à la norme EN12897","(2) - Perte de chaleur conforme à la norme EN12897","(2) - Perte de chaleur conforme à la norme EN12897","(2) - Perte de chaleur conforme à la norme EN12897"]
["","","","","","(3) - Pour en savoir plus, se reporter au schéma de plage de fonctionnement.","(3) - Pour en savoir plus, se reporter au schéma de plage de fonctionnement.","(3) - Pour en savoir plus, se reporter au schéma de plage de fonctionnement.","(3) - Pour en savoir plus, se reporter au schéma de plage de fonctionnement."]