{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DV"]
[]
[]
[]
[]
["","","","","","ERLA03DAV3"]
["Dimensions","Unité","","Hauteur","mm","550"]
["","","","Largeur","mm","765"]
["","","","Profondeur","mm","285"]
["Poids","Unité","","","kg","35"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","32.0"]
["","","Rafraîchissement","Haut","m³/min","36"]
["Plage de fonct.","Rafraîch.","","Min.","°CBS","10"]
["","","","Max.","°CBS","43"]
["Plage de fonctionnement","Eau chaude domestique","","Min.","°CBS","-15"]
["Plage de fonct.","Eau chaude sanitaire","","Max.","°CBS","35"]
["Niveau de puissance sonore","Chauffage","","Nom.","dBA","59"]
["","Rafraîchissement","","Nom.","dBA","60"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","46"]
["","Rafraîchissement","","Nom.","dBA","46"]
["Réfrigérant","Type","","","","R-32"]
["Réfrigérant","PRP","","","","675.0"]
["Réfrigérant","Charge","","","tCO2Eq","0.675"]
["","Charge","","","kg","1"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["Raccords de tuyauterie","Gaz","","DE","mm","9.52"]
["Raccords de tuyauterie","Dénivelé","UI - UE","Max.","m","20.0"]
["Alimentation électrique","Nom","","","","V3"]
["","Phase","","","","1N~"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","50"]
["","Alimentation électrique-=-Tension","","Alimentation électrique-=-Tension-=-V","","220-240"]
["Courant","Current-=-Recommended fuses","","Fusibles recommandés","","16"]
["Remarques","","","","","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]