{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERSQ-AY1"]
[]
[]
[]
[]
["","","","","","ERSQ011AAY1","ERSQ014AAY1","ERSQ016AAY1"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","52","53","55"]
["Accessoires standard","Manuel d'installation","","","","1","1","1"]
["Réfrigérant","PRP","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","4.5","4.5","4.5"]
["","Type","","","","R-410A","R-410A","R-410A"]
["Plage de fonctionnement","Chauffage","","Max.","°CBH","20","20","20"]
["","","","Min.","°CBH","-20","-20","-20"]
["","Eau chaude domestique","","Min.","°CBS","-20","-20","-20"]
["","","","Max.","°CBS","35","35","35"]
["Raccords de tuyauterie","Isolation thermique","","","","Tuyaux de liquide et tuyaux de gaz","Tuyaux de liquide et tuyaux de gaz","Tuyaux de liquide et tuyaux de gaz"]
["","Liquide","","DE","mm","9.52","9.52","9.52"]
["","Gaz","","DE","mm","15.9","15.9","15.9"]
["","Évacuation","","DE","mm","26x3","26x3","26x3"]
["","Dénivelé","UI - UE","Max.","m","30","30","30"]
["Sound power level","Heating","","Nom.","dBA","68","69","71"]
["Dimensions","Unité","","Largeur","mm","900","900","900"]
["","","","Profondeur","mm","320","320","320"]
["","","","Hauteur","mm","1,345","1,345","1,345"]
["Poids","Unité","","","kg","120","120","120"]
["Power supply","Phase","","","","3~","3~","3~"]
["","Nom","","","","Y1","Y1","Y1"]
["","Fréquence","","","Hz","50","50","50"]
["","Tension","","","V","380-415","380-415","380-415"]
["Courant","Fusibles recommandés","","","A","16","16","16"]
["Remarques","","","","","(1) - Voir le schéma séparé pour la plage de fonctionnement","(1) - Voir le schéma séparé pour la plage de fonctionnement","(1) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","(2) - Ssc : puissance de court-circuit","(2) - Ssc : puissance de court-circuit","(2) - Ssc : puissance de court-circuit"]
["","","","","","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés.","(3) - Contient des gaz à effet de serre fluorés."]