{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERWQ-AV3"]
[]
[]
[]
[]
["","","","","","ERWQ02AAV3"]
["Dimensions","Unité","","Hauteur","mm","550"]
["","","","Largeur","mm","765"]
["","","","Profondeur","mm","285"]
["Poids","Unité","","","kg","35"]
["Plage de fonctionnement","Eau chaude sanitaire","","Max.","°CBS","35"]
["","","","Min.","°CBS","-15"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","9.5"]
["","Dénivelé","UI - UE","Max.","m","15"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","47"]
["","Rafraîchissement","","Nom.","dBA","47"]
["Réfrigérant","Type","","","","R-410A"]
["","PRP","","","","2,087.5"]
["","Charge","","","kg","1.05"]
["Power supply","Nom","","","","V3"]
["","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","230"]
["Remarques","","","","","(1) - Contient des gaz à effet de serre fluorés."]