{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH-D"]
[]
[]
[]
[]
["","","","","","ETSH16P50DA","ETSH16P30DA"]
["Niveau de pression sonore","Nom.","","","dBA","32.8","32.8"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","10","10"]
["","","Côté eau","Max.","°C","22","22"]
["","","","Min.","°C","5","5"]
["","Chauffage","Côté eau","Max.","°C","70","70"]
["","","","Min.","°C","15","15"]
["Niveau de puissance sonore","Nom.","","","dBA","45.6","45.6"]
["Dimensions","Unité","","Largeur","mm","785","590"]
["","","","Profondeur","mm","785","615"]
["","","","Hauteur","mm","1,896","1,891"]
["Caisson","Matériau","","","","Polypropylène anti-choc","Polypropylène anti-choc"]
["","Colour","","","","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)","Blanc signalisation (RAL9016) / Gris foncé (RAL7011)"]
["DESP","Catégorie","","","","Art 4.3","Art 4.3"]
["Poids","Unité","","","kg","90","73"]
["Power supply","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Tension","","","V","230","230"]
["Dispositif de chauffage électrique","Alimentation électrique","","Fréquence","Hz","50","50"]
["","","","Nom","","3V / 9W","3V / 9W"]
["","","","Phase","","1~ / 3~","1~ / 3~"]
["Remarques","","","","","(1) - Perte de chaleur conforme à la norme EN12897","(1) - Perte de chaleur conforme à la norme EN12897"]
["","","","","","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C"]
["","","","","","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60 ℃","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60 ℃"]
["","","","","","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65 ℃","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65 ℃"]