{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-F"]
[]
[]
[]
[]
["","","","","FCQG60FVEB / RXS60F3V1B","FCQG60FVEB / RXS60F4V1B"]
["Puissance frigorifique","Nom.","","kW","5.70 (3)","5.70"]
["Raccords de tuyauterie","Liquide","DE","mm","","6.35"]
["","Gaz","DE","mm","","12.7"]
["","Évacuation","OD","mm","","VP20 (diamètre ext. : 26 / diamètre int. : 20)"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","820","820"]
["","EER","","","3.48","3.48"]
["","COP","","","3.52","3.52"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","B","B"]
["Puissance calorifique","Nom.","","kW","7.00 (4)","7.00"]
["Remarques","","","","(1) - Étiquette énergétique : échelle de A (efficacité maximum) à G (efficacité minimum).","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - Consommation énergétique annuelle : basée sur un fonctionnement moyen de 500 heures par an à pleine charge (conditions nominales)","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]
["","","","","(3) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 5m ; dénivelé : 0m"]
["","","","","(4) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m ; dénivelé : 0m"]
["","","","","(5) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]