{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Puissance frigorifique","Puissance totale","","Nom.","kW","12.10","19.00","22.00"]
["Puissance calorifique","Puissance totale","","Nom.","kW","13.50","22.4","24.0"]
["Caisson","Couleur","","","","Non peint","Non peint","Non peint"]
["","Matériau","","","","Acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","300","470","470"]
["","","","Largeur","mm","1,400","1,490","1,490"]
["","","","Profondeur","mm","700","1,100","1,100"]
["Poids","Unité","","","kg","45","104","115"]
["Vide de faux-plafond requis >","mm","","","","350"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","39.0","64.0","69.0"]
["","","","Moyen","m³/min","","50","56"]
["","","","Bas","m³/min","28.0","36.0","43.0"]
["","","Chauffage","Haut","m³/min","39.0","64.0","69.0"]
["","","","Moyen","m³/min","","50.0","56.0"]
["","","","Bas","m³/min","28.0","36.0","43.0"]
["","Pression statique externe","","Haute","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Sound power level","Rafraîchissement","","","dBA","66","69.0","71.0"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","40","43.0","44.0"]
["","","","Moyen","dBA","","39.0","40.0"]
["","","","Bas","dBA","33","36.0","37.0"]
["","Chauffage","","Haut","dBA","40","43.0","44.0"]
["","","","Moyen","dBA","","39.0","40.0"]
["","","","Bas","dBA","33","36.0","37.0"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52","9.52","9.52"]
["","Gaz","","DE","mm","15.90","19.1","22.2"]
["","Évacuation","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Hauteur manométrique","mm","","","","625"]
["Panneau décoratif","Modèle","","","","BYBS125DJW1"]
["","Couleur","","","","Blanc (10Y9/0,5)"]
["","Dimensions","","Hauteur","mm","55"]
["","","","Largeur","mm","1,500"]
["","","","Profondeur","mm","500"]
["","Poids","","","kg","6.5"]
["Systèmes de commande","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Télécommande câblée","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Accessoires standard","Vis","","","","16","2","2"]
["","Rondelle","","","","8","12","12"]
["","Collier de serrage","","","","1"]
["","Flexible d'évacuation","","","","1"]
["","Précautions générales de sécurité","","","","1","1","1"]
["","Manuel d'installation et d'exploitation","","","","1","1","1"]
["","Câble pour alimentation commune","","","","2"]
["","Matériau d’étanchéité (flexible d’évacuation)","","","","1"]
["","Matériau d'étanchéité","","","","2"]
["","Tube d'isolation thermique (liquide)","","","","1"]
["","Tube d’isolation thermique (gaz)","","","","1"]
["Power supply","Nom","","","","","VE","VE"]
["","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50/60","50/60","50/60"]
["","Tension","","","V","220-240/220","220-240/220","220-240/220"]
["Remarques","","","","","(1) - Pour les données électriques, se reporter au schéma séparé."]
["Accessoires standard","Manuel d’utilisation","","","","","1","1"]
["","Manuel d'installation","","","","","1","1"]
["","Tuyau de raccordement de gaz","","","","","1","1"]
["","Attache-câble","","","","","1","1"]
["","Rondelle à ressort","","","","","2","2"]
["","Vis+Rondelle","","","","","45","45"]
["","Vis à tête hexagonale avec rondelle","","","","","49","49"]
["","Vis à tête hexagonale","","","","","2","2"]
["","Rondelle plate","","","","","8","8"]