{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","35.0","35.0"]
["","","","Bas","dBA","29.0","29.0"]
["","Rafraîchissement","","Bas","dBA","28.0","28.0"]
["","","","Haut","dBA","35.0","35.0"]
["Accessoires standard","Manuel d'installation et d'exploitation","","","","1","1"]
["","Filtre d'air d'aspiration","","","","1","1"]
["Systèmes de contrôle","Télécommande câblée","","","","BRC1D52, BRC1E52A/B"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","9.52"]
["","Évacuation","","","","27.2"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","55","55"]
["","Chauffage","","","dBA","55","55"]
["Dimensions","Unité","","Largeur","mm","652","652"]
["","","","Profondeur","mm","502","502"]
["","","","Hauteur","mm","230","230"]
["Caisson","Matériau","","","","Acier zingué à faible teneur en carbone","Acier zingué à faible teneur en carbone"]
["Poids","Unité","","","kg","17.0","17.0"]
["Ventilateur","Débit d’air","Chauffage","Haut","m³/min","","6.95"]
["","","","Bas","m³/min","","5.20"]
["","","Rafraîchissement","Bas","m³/min","","5.20"]
["","","","Haut","m³/min","","6.50"]
["Power supply","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Nom","","","","V1","V1"]
["","Tension","","","V","230","230 +/-10%"]
["Remarques","","","","","(1) - Les valeurs sonores sont mesurées en salle semi-anéchoïque.","(1) - Les valeurs sonores sont mesurées en salle semi-anéchoïque."]
["","","","","","(2) - Il s'agit d'une valeur relative qui varie en fonction de la distance et de l'environnement acoustique. Pour plus de détails, se reporter aux schémas de niveau sonore.","(2) - Il s'agit d'une valeur relative qui varie en fonction de la distance et de l'environnement acoustique. Pour plus de détails, se reporter aux schémas de niveau sonore."]
["","","","","","(3) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(3) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore."]
["Raccords de tuyauterie","Liquide","","DE","mm","","6.35"]
["","Gaz","","DE","mm","","9.52"]
["","Évacuation","","","","","27.2"]