{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB / RZQSG125L9V1B (Archived)","FDQ125C7VEB / RZQSG125L9V1B (Archived)"]
["Puissance frigorifique","Nom.","","kW","12.0","12.0"]
["Puissance calorifique","Nom.","","kW","13.5","13.5"]
["Efficacité nominale","EER","","","3.21","3.21"]
["","COP","","","3.51","3.51"]
["","Consommation énergétique annuelle","","kWh","1,870","1,870"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","B","B"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A","A"]
["","Puissance","Pdesign","kW","12.00","12.00"]
["","SEER","","","5.20","5.20"]
["","Consommation d’énergie annuelle","","kWh/a","808","808"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A","A"]
["","Puissance","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.90","3.90"]
["","Consommation d’énergie annuelle","","kWh/a","2,729","2,729"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]