{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","35.0","35.0","","38.0"]
["","","","Moyen","dBA","33.0","33.0","","35.0"]
["","","","Bas","dBA","27.0","27.0","","30.0"]
["","Rafraîchissement","","Moyen","dBA","33.0","33.0","","35.0"]
["","","","Bas","dBA","27.0","27.0","","30.0"]
["","","","Haut","dBA","35.0","35.0","","38.0"]
["Accessoires standard","Manuel d'installation","","","","1","1","","1"]
["","Manuel d’utilisation","","","","1","1","","1"]
["","Isolant pour raccord","","","","1","1","","1"]
["","Tampon d’étanchéité","","","","1","1","","1"]
["","Attache métallique","","","","1","1","","1"]
["","Flexible d'évacuation","","","","1","1","","1"]
["","Rondelle pour attache de suspension","","","","8","8","","8"]
["","Matériau d'étanchéité","","","","2","2","","2"]
["","Attaches","","","","6","6","","6"]
["","Plaque de fixation à rondelle","","","","4","4","","4"]
["","Vis de brides à gaines","","","","1","1","","1"]
["","Filtre à air","","","","1","1","","1"]
["Piping connections","Liquide","","DE","mm","6.35","6.35","","6.35"]
["","Gaz","","DE","mm","9.50","9.50","","12.70"]
["","Évacuation","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.036","0.036","","0.060"]
["","Chauffage","","Nom.","kW","0.036","0.036","","0.060"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","53.0","53.0","","56.0"]
["","Chauffage","","","dBA","53.0","53.0","","56.0"]
["Dimensions","Unité","","Largeur","mm","750","750","","1,150"]
["","","","Profondeur","mm","620","620","","620"]
["","","","Hauteur","mm","200","200","","200"]
["Poids","Unité","","","kg","21","21","","28"]
["Ventilateur","Pression statique externe","","Nom.","Pa","30","30","","40"]
["","Débit d'air","Chauffage","Haut","m³/min","8.7","8.7","","16.0"]
["","","","Moyen","m³/min","8.0","8.0","","14.8"]
["","","","Bas","m³/min","7.3","7.3","","13.5"]
["","","Rafraîchissement","Bas","m³/min","7.3","7.3","","13.5"]
["","","","Moyen","m³/min","8.0","8.0","","14.8"]
["","","","Haut","m³/min","8.7","8.7","","16.0"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Fréquence","","","Hz","50","50","","50"]
["","Tension","","","V","220-240","220-240","","220-240"]
["Remarques","","","","","(1) - Pour les données électriques, se reporter au schéma séparé.","(1) - Pour les données électriques, se reporter au schéma séparé.","","(1) - Pour les données électriques, se reporter au schéma séparé."]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","","0.060"]
["","Chauffage","","Nom.","kW","","","0.060"]
["Dimensions","Unité","","Hauteur","mm","","","200"]
["","","","Largeur","mm","","","1150"]
["","","","Profondeur","mm","","","620"]
["Poids","Unité","","","kg","","","28"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","","15.8"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","","14.6"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","","13.3"]
["","","Chauffage","Haut","m³/min","","","15.8"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","","14.6"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","","13.3"]
["","Pression statique externe","","Nom.","Pa","","","40"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","","55.0"]
["","Chauffage","","","dBA","","","55.0"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","","38.0"]
["","Refroidissement","","Moyen","dBA","","","35.0"]
["","","","Bas","dBA","","","30.0"]
["","Chauffage","","Haut","dBA","","","38.0"]
["","","","Moyen","dBA","","","35.0"]
["","","","Bas","dBA","","","30.0"]
["Raccords de tuyauterie","Liquide","","DE","mm","","","6.35"]
["","Gaz","","DE","mm","","","12.70"]
["","Évacuation","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Accessoires standard","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Filtre à air","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Alimentation électrique","Phase","","","","","","1~"]
["","Fréquence","","","Hz","","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","","220-240"]