{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-D"]
[]
[]
[]
[]
["","","","","","FTXC20DV1B","FTXC25DV1B","FTXC35DV1B","FTXC50DV1B","FTXC60DV1B","FTXC71DV1B"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.595","0.765","1.05","1.55","1.89","2.38"]
["","Chauffage","","Nom.","kW","0.670","0.750","1.07","1.52","1.68","2.46"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc","Blanc","Blanc","Blanc"]
["","Matériau","","","","Polystyrène à fort impact","Polystyrène à fort impact","Polystyrène à fort impact","Polystyrène à fort impact","Polystyrène à fort impact","Polystyrène à fort impact"]
["Dimensions","Unité","","Hauteur","mm","288","288","288","288","297","297"]
["","","","Largeur","mm","770","770","770","770","990","990"]
["","","","Profondeur","mm","234","234","234","234","273","273"]
["Poids","Unité","","","kg","9.00","9.00","9.50","9.50","13.0","13.0"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","10.8","10.8","11.1","12.5","20.4","20.4"]
["","","","Moyen","m³/min","8.1","8.1","8.7","9.9","14.5","14.5"]
["","","","Bas","m³/min","6.1","6.1","6.4","8.1","12.5","12.5"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.4","5.4","5.4","7.4","10.2","10.2"]
["Sound power level","Rafraîchissement","","","dBA","57","57","58","60","63","63"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","40","40","41","47","48","48"]
["","","","Moyen","dBA","33","33","34","39","42","42"]
["","","","Bas","dBA","26","26","26","33","38","38"]
["","","","Faible niveau sonore de fonctionnement","dBA","21","21","22","30","31","31"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.52","9.52","9.52","12.7","12.7","12.7"]
["","Évacuation","","","","16.5","16.5","16.5","16.5","16.5","16.5"]
["Systèmes de contrôle","Infrared remote control","","","","ARC486A2","ARC486A2","ARC486A2","ARC486A2","ARC486A2","ARC486A2"]
["Power supply","Nom","","","","V1","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50","50"]
["","Tension","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]