{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXD-A / RXD-A"]
[]
[]
[]
[]
["","","","","FTXD25A5V1B / RXD25A5V1B","FTXD35A5V1B / RXD35A5V1B"]
["Unité extérieure","","","","RXD25A5V1B","RXD35A5V1B"]
["Puissance frigorifique","Min.","","kW","1.3","1.4"]
["","Nom.","","kW","2.5","3.3"]
["","Max.","","kW","3.2","3.9"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","1.3","1.4"]
["","Nom.","","kW","2.8","3.5"]
["","Max.","","kW","4.4","5"]
["Efficacité nominale","EER","","","4.46","4.23"]
["","COP","","","4.59","3.98"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A+++","A+++"]
["","Puissance","Pdesign","kW","2.5","3.3"]
["","SEER","","","8.5","8.5"]
["","Consommation d’énergie annuelle","","kWh/a","103","136"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A+++","A+++"]
["","Puissance","Pdesign","kW","2.4","2.5"]
["","SCOP/A","","","5.1","5.1"]
["","Pdh Puissance calorifique à -10°","","kW","2.12","2.19"]
["","Consommation d’énergie annuelle","","kWh/a","659","686"]
["Remarques","","","","(1) - Pour les données électriques, se reporter au schéma séparé.","(1) - Pour les données électriques, se reporter au schéma séparé."]
["","","","","(2) - Puissances frigo. nominales basées sur: température int. : 27°CBS, 19°CBH, température ext.: 35°CBS, tuyauterie de réfrig. équiv.: 5 m, diff. de niveau: 0 m. Données pour séries d'effic. standard, certif. Eurovent","(2) - Puissances frigo. nominales basées sur: température int. : 27°CBS, 19°CBH, température ext.: 35°CBS, tuyauterie de réfrig. équiv.: 5 m, diff. de niveau: 0 m. Données pour séries d'effic. standard, certif. Eurovent"]
["","","","","(3) - Puissances calo. nominales basées sur: température int. : 20°CBS, température ext.: 7°CBS, 6°CBH, tuyauterie de réfrig. équiv.: 5 m, diff. de niveau: 0 m. Données pour séries d'effic. standard","(3) - Puissances calo. nominales basées sur: température int. : 20°CBS, température ext.: 7°CBS, 6°CBH, tuyauterie de réfrig. équiv.: 5 m, diff. de niveau: 0 m. Données pour séries d'effic. standard"]