{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-K"]
[]
[]
[]
[]
["","","","","FTXM20K3V1B (Archived)","FTXM25K3V1B (Archived)","FTXM35K3V1B (Archived)","FTXM42K3V1B (Archived)","FTXM50K3V1B (Archived)"]
["Niveau de pression sonore","Chauffage","Haut","dBA","40","41","45","45","47"]
["","","Faible niveau sonore de fonctionnement","dBA","19","19","19","22","24"]
["","","Bas","dBA","27","27","29","33","34"]
["","Rafraîchissement","Faible niveau sonore de fonctionnement","dBA","19","19","19","21","23"]
["","","Bas","dBA","24","25","29","33","34"]
["","","Haut","dBA","40","41","45","45","46"]
["","","Nom.","dBA","34","34","39","39","40"]
["","Rafraîchissement","Nom.","dBA","32","33","37","39","40"]
["Accessoires standard","Manuel d’utilisation","","","1","1","1","1","1"]
["","Manuel d'installation","","","1","1","1","1","1"]
["","Télécommande infrarouge","","","1","1","1","1","1"]
["","Piles","","","2","2","2","2","2"]
["","Plaque de montage","","","1","1","1","1","1"]
["","Vis de fixation d'unité intérieure","","","2","2","2","2","2"]
["","Filtre purificateur d'air photocatalytique à apatite de titane","","","2","2","2","2","2"]
["","Support de télécommande","","","1","1","1","1","1"]
["Systèmes de contrôle","Infrared remote control","","","ARC466A6","ARC466A6","ARC466A9","ARC466A9","ARC466A9"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gaz","DE","mm","9.5","9.5","9.5","12.7","12.7"]
["","Évacuation","","","18","18","18","18","18"]
["Sound power level","Rafraîchissement","","dBA","56","57","59","59","60"]
["","Chauffage","","dBA","56","57","59","59","60"]
["Dimensions","Unité","Largeur","mm","780","780","900","900","900"]
["","","Profondeur","mm","215","215","215","215","215"]
["","","Hauteur","mm","289","289","298","298","298"]
["Caisson","Couleur","","","Blanc","Blanc","Blanc","Blanc","Blanc"]
["Poids","Unité","","kg","8","8","11","11","11"]
["Power supply","Phase","","","1~","1~","1~","1~","1~"]
["","Fréquence","","Hz","50","50","50","50","50"]
["","Nom","","","V1","V1","V1","V1","V1"]
["","Tension","","V","220-240","220-240","220-240","220-240","220-240"]
["Remarques","","","","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230 V","(3) - 230 V","(3) - 230 V","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V","(4) - 240V"]