{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RXM-A9"]
[]
[]
[]
[]
["","","","","FTXM25R2V1B / RXM25A5V1B9","FTXM25R5V1B / RXM25A5V1B9","FTXM35R2V1B / RXM35A5V1B9","FTXM35R5V1B / RXM35A5V1B9","FTXM50R2V1B / RXM50A5V1B9"]
["Puissance frigorifique","Min.","","kW","1.3","1.3","1.4","1.4","1.7"]
["","Nom.","","kW","2.5","2.5","3.4","3.4","5"]
["","Max.","","kW","3.2","3.2","4","4","6"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","1.3","1.3","1.4","1.4","1.7"]
["","Nom.","","kW","2.8","2.8","4","4","5.8"]
["","Max.","","kW","4.7","4.7","5.2","5.2","7.7"]
["Efficacité nominale","EER","","","4.5","4.5","4.23","4.23","3.68"]
["","COP","","","5","5","4.04","4.04","4"]
["","Consommation énergétique annuelle","","kWh","278","278","402","402","679"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A","A","A","A"]
["","","Chauffage","","A","A","A","A","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A+++","A+++","A+++","A+++","A++"]
["","Puissance","Pdesign","kW","2.5","2.5","3.4","3.4","5"]
["","SEER","","","8.65","8.65","8.65","8.65","7.41"]
["","Consommation d’énergie annuelle","","kWh/a","101","101","137","137","236"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A+++","A+++","A+++","A+++","A++"]
["","Puissance","Pdesign","kW","2.4","2.4","2.5","2.5","4.6"]
["","SCOP/A","","","5.1","5.1","5.1","5.1","4.71"]
["","Pdh Puissance calorifique à -10°","","kW","2.3","2.3","2.35","2.35","3.85"]
["","Consommation d’énergie annuelle","","kWh/a","659","659","686","686","1368"]
["Remarques","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(3) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(3) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(3) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]