{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM40A2V1B9","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM50A2V1B9"]
["Puissance frigorifique","Nom.","","kW","4"]
["Puissance calorifique","Nom.","","kW","4.2"]
["Efficacité nominale","EER","","","3.71"]
["","COP","","","3.75"]
["","Consommation énergétique annuelle","","kWh","539"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A"]
["","","Chauffage","","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A++"]
["","Puissance","Pdesign","kW","4"]
["","SEER","","","7.74"]
["","Consommation d’énergie annuelle","","kWh/a","181"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A+"]
["","Puissance","Pdesign","kW","3.2"]
["","SCOP/A","","","4.3"]
["","Pdh Puissance calorifique à -10°","","kW","2.46"]
["","Consommation d’énergie annuelle","","kWh/a","1041"]
["Remarques","","","","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(1) - Les puissances frigorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["","","","","(3) - See separate drawing for operation range","(3) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","(4) - See separate drawing for electrical data","(4) - Pour les données électriques, se reporter au schéma séparé."]
["Puissance frigorifique","Nom.","","kW","","4.00"]
["Puissance calorifique","Nom.","","kW","","5.20"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","","554"]
["","COP","","","","3.68"]
["","EER","","","","3.61"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","A"]
["","","Chauffage","","","A"]