{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS71GV1B","FTXS60GV1B (Archived)"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","38","39","42","42","44","46"]
["","","","Faible niveau sonore de fonctionnement","dBA","25","25","26","30","31","34"]
["","","","Bas","dBA","28","28","29","33","34","37"]
["","Rafraîchissement","","Faible niveau sonore de fonctionnement","dBA","22","22","23","30","31","34"]
["","","","Bas","dBA","25","25","26","33","34","37"]
["","","","Haut","dBA","38","38","42","42","43","46"]
["","","","Nom.","dBA","33","34","36","38","39","42"]
["","Rafraîchissement","","Nom.","dBA","32","32","34","38","39","42"]
["Accessoires standard","Filtre purificateur d'air photocatalytique à apatite de titane","","","","2","2","2","2","2"]
["","Manuel d’utilisation","","","","1","1","1","1","1","1"]
["","Manuel d'installation","","","","1","1","1","1","1","1"]
["","Télécommande infrarouge","","","","1","1","1","1","1","1"]
["","Piles","","","","2","2","2","2","2","2"]
["","Support de télécommande","","","","1","1","1","1","1","1"]
["","Vis de fixation d'unité intérieure","","","","2","2","2","2","2","2"]
["","Plaque de montage","","","","1","1","1","1","1","1"]
["Systèmes de contrôle","Infrared remote control","","","","","","","","","ARC452A3"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.52","9.52","9.52","9.52","12.70","15.9"]
["","Évacuation","","","","18","18","18","18","18","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Chauffage","","Nom.","kW","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Sound power level","Rafraîchissement","","","dBA","54","54","58","58","59","63"]
["","Chauffage","","","dBA","54","55","58","58","60","62"]
["Dimensions","Unité","","Largeur","mm","800","800","800","800","800","1,050"]
["","","","Profondeur","mm","215","215","215","215","215","250"]
["","","","Hauteur","mm","295","295","295","295","295","290"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc","Blanc","Blanc","Blanc"]
["Poids","Unité","","","kg","9","9","10","10","10","12"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50","50"]
["","Nom","","","","V1","V1","V1","V1","V1","V1"]
["","Tension","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Remarques","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230 V","(3) - 240V"]
["Accessoires standard","Filtre purificateur d'air photocatalytique à apatite de titane sans armature","","","","","","","","","2"]
["Remarques","","","","","","","","","","(4) - 240V"]
["Ventilateur","Débit d'air","Rafraîchissement","Nom.","m³/min","","","","","","","16.0"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","","","","","","","41"]
["Ventilateur","Débit d'air","Chauffage","Nom.","m³/min","","","","","","","14.9"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","","","","","","","40"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Chauffage","","Nom.","kW","","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Caisson","Couleur","","","","","","","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","","","","","","","290"]
["","","","Largeur","mm","","","","","","","1050"]
["","","","Profondeur","mm","","","","","","","250"]
["Poids","Unité","","","kg","","","","","","","12"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","","","","","","16.0"]
["","","","Bas","m³/min","","","","","","","11.3"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","","","","","","10.1"]
["","","Chauffage","Haut","m³/min","","","","","","","17.2"]
["","","","Bas","m³/min","","","","","","","12.6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","","","","","","11.3"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","","","","","","60"]
["","Chauffage","","","dBA","","","","","","","59"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","","","","","","45"]
["","","","Bas","dBA","","","","","","","36"]
["","","","Faible niveau sonore de fonctionnement","dBA","","","","","","","33"]
["","Chauffage","","Haut","dBA","","","","","","","44"]
["","","","Bas","dBA","","","","","","","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","","","","","","","32"]
["Raccords de tuyauterie","Liquide","","DE","mm","","","","","","","6.35"]
["","Gaz","","DE","mm","","","","","","","12.7"]
["","Évacuation","","","","","","","","","","18"]
["Systèmes de commande","Télécommande infrarouge","","","","","","","","","","ARC452A3"]
["Accessoires standard","Installation manual","","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","","1"]
["","Operation manual","","","","","","","","","","1"]
["","Batteries","","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","","2"]
["Alimentation électrique","Nom","","","","","","","","","","V1"]
["","Phase","","","","","","","","","","1~"]
["","Fréquence","","","Hz","","","","","","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","","","","","","220-240"]