{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BB"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BB"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","41"]
["","","","Moyen","dBA","31"]
["","","","Faible niveau sonore de fonctionnement","dBA","19"]
["","","","Bas","dBA","24"]
["","Rafraîchissement","","Moyen","dBA","32"]
["","","","Faible niveau sonore de fonctionnement","dBA","20"]
["","","","Bas","dBA","25"]
["","","","Haut","dBA","43"]
["Accessoires standard","Manuel d'installation","","","","1"]
["","Manuel d’utilisation","","","","1"]
["","Filtre à air","","","","2"]
["","Télécommande infrarouge","","","","1"]
["","Plaque de montage de télécommande","","","","1"]
["","Sachet de vis","","","","1"]
["","Cache de vis","","","","2"]
["","Piles sèches AAA","","","","2"]
["","Précautions générales de sécurité","","","","1"]
["Réfrigérant","PRP","","","","675.0"]
["Systèmes de commande","Wired remote control","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","9.50"]
["","Drain","","","","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.023"]
["","Chauffage","","Nom.","kW","0.022"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","60"]
["","Chauffage","","","dBA","60"]
["Dimensions","Unité","","Largeur","mm","798"]
["","","","Profondeur","mm","189"]
["","","","Hauteur","mm","295"]
["Caisson","Colour","","","","Noir"]
["Poids","Unité","","","kg","11.5"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","11.5"]
["","","","Bas","m³/min","6.0"]
["","","","Moyen","m³/min","8.0"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.1"]
["","","Rafraîchissement","Bas","m³/min","5.7"]
["","","","Moyen","m³/min","8.3"]
["","","","Haut","m³/min","11.9"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.6"]
["Power supply","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Nom","","","","V1"]
["","Tension","","","V","220-240"]
["Remarques","","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m"]
["","","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m"]
["","","","","","(3) - Pour les données électriques, se reporter au schéma séparé."]