{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A / RXTM-A"]
[]
[]
[]
[]
["","","","","FTXTM30A2V1B / RXTM30A2V1B","FTXTM40A2V1B / RXTM40A2V1B"]
["Puissance frigorifique","Min.","","kW","1.2","1.2"]
["","Nom.","","kW","3","4"]
["","Max.","","kW","4.6","5.2"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","0.8","0.9"]
["","Nom.","","kW","3.2","4"]
["","Max.","","kW","7.4","8.8"]
["Efficacité nominale","EER","","","5.13","4.71"]
["","COP","","","5.3","5.51"]
["","Consommation énergétique annuelle","","kWh","292","425"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A+++","A+++"]
["","Puissance","Pdesign","kW","3","4"]
["","SEER","","","8.65","8.95"]
["","Consommation d’énergie annuelle","","kWh/a","121","156"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A+++","A+++"]
["","Puissance","Pdesign","kW","3","3.8"]
["","SCOP/A","","","5.35","5.5"]
["","Pdh Puissance calorifique à -10°","","kW","3","3.8"]
["","Consommation d’énergie annuelle","","kWh/a","785","967"]
["Classe d'efficacité énergétique","","","","A+++ ~ D","A+++ ~ D"]
["Remarques","","","","(1) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes: température intérieure: 20°CBS; température extérieure: 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente: 5m, dénivelé: 0m.","(1) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes: température intérieure: 20°CBS; température extérieure: 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente: 5m, dénivelé: 0m."]
["","","","","(2) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes: température intérieure: 27°CBS, 19°CBH; température extérieure: 35°CBS ; longueur équivalente de tuyauterie de réfrigérant: 5m, dénivellation: 0m.","(2) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes: température intérieure: 27°CBS, 19°CBH; température extérieure: 35°CBS ; longueur équivalente de tuyauterie de réfrigérant: 5m, dénivellation: 0m."]
["","","","","(3) - Voir le schéma séparé pour la plage de fonctionnement","(3) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","(4) - Pour les données électriques, se reporter au schéma séparé.","(4) - Pour les données électriques, se reporter au schéma séparé."]