{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.029","0.053"]
["","Chauffage","","Nom.","kW","0.024","0.06"]
["Caisson","Couleur","","","","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","298","298"]
["","","","Largeur","mm","804","997"]
["","","","Profondeur","mm","252","292"]
["Poids","Unité","","","kg","12","15"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","13.2","15.1"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","8.1","9.2"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","5.6","5.6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.8","4.8"]
["","","Chauffage","Haut","m³/min","11.7","17"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","7.7","10"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","5.6","6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.7","5.1"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","60","60"]
["","Chauffage","","","dBA","59","60"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","45","46"]
["","Refroidissement","","Moyen","dBA","33","32"]
["","","","Bas","dBA","25","24"]
["","","","Faible niveau sonore de fonctionnement","dBA","21","20"]
["","Chauffage","","Haut","dBA","43","46"]
["","","","Moyen","dBA","31","31"]
["","","","Bas","dBA","22","22"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19"]
["Réfrigérant","Réfrigérant-=-PRP","","","","675","675"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35"]
["","Gaz","","DE","mm","9.5","9.5"]
["","Évacuation","","","","18","18"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC466A83","ARC466A83"]
["Accessoires standard","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentation électrique","Nom","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240"]
["Remarques","","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m"]
["","","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m"]
["","","","","","(3) - Pour les données électriques, se reporter au schéma séparé.","(3) - Pour les données électriques, se reporter au schéma séparé."]
["Accessoires standard","FTXTM40A2V1B","","","","","1"]